##
## This file is part of the coreboot project.
## 
## Copyright (C) 2007-2008 coresystems GmbH
##
## This program is free software; you can redistribute it and/or
## modify it under the terms of the GNU General Public License as
## published by the Free Software Foundation; version 2 of
## the License.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston,
## MA 02110-1301 USA
##

# Tables
uses HAVE_MP_TABLE
uses HAVE_PIRQ_TABLE
uses IRQ_SLOT_COUNT
uses HAVE_OPTION_TABLE
uses USE_OPTION_TABLE
uses LB_CKS_RANGE_START
uses LB_CKS_RANGE_END
uses LB_CKS_LOC
uses HAVE_ACPI_TABLES
uses HAVE_ACPI_RESUME
uses HAVE_MAINBOARD_RESOURCES
uses HAVE_HIGH_TABLES
# SMP
uses CONFIG_SMP
uses CONFIG_LOGICAL_CPUS
uses CONFIG_AP_IN_SIPI_WAIT
uses CONFIG_MAX_CPUS
uses CONFIG_MAX_PHYSICAL_CPUS
uses CONFIG_IOAPIC
# Image Size
uses USE_FALLBACK_IMAGE
uses HAVE_FALLBACK_BOOT
uses FALLBACK_SIZE
uses ROM_SIZE
uses ROM_SECTION_SIZE
uses ROM_IMAGE_SIZE
uses ROM_SECTION_SIZE
uses ROM_SECTION_OFFSET
# Payload
uses CONFIG_ROM_PAYLOAD
uses CONFIG_ROM_PAYLOAD_START
uses CONFIG_COMPRESSED_PAYLOAD_LZMA
uses CONFIG_PRECOMPRESSED_PAYLOAD
uses PAYLOAD_SIZE
# Build Internals
uses _RAMBASE
uses _ROMBASE
uses STACK_SIZE
uses HEAP_SIZE
uses USE_DCACHE_RAM
uses DCACHE_RAM_BASE
uses DCACHE_RAM_SIZE
uses CONFIG_USE_INIT
uses CONFIG_USE_PRINTK_IN_CAR
uses XIP_ROM_BASE
uses XIP_ROM_SIZE
uses HAVE_HARD_RESET
uses HAVE_SMI_HANDLER
uses CONFIG_PCIE_CONFIGSPACE_HOLE
uses MMCONF_SUPPORT
uses MMCONF_BASE_ADDRESS
uses CONFIG_GFXUMA
uses CONFIG_CBFS

#
uses MAINBOARD
uses MAINBOARD_PART_NUMBER
uses MAINBOARD_VENDOR
uses MAINBOARD_PCI_SUBSYSTEM_VENDOR_ID
uses MAINBOARD_PCI_SUBSYSTEM_DEVICE_ID
# Timers
uses CONFIG_UDELAY_TSC
uses CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2
# Console
uses CONFIG_CONSOLE_SERIAL8250
uses TTYS0_BAUD
uses TTYS0_BASE
uses TTYS0_LCS
uses DEFAULT_CONSOLE_LOGLEVEL
uses MAXIMUM_CONSOLE_LOGLEVEL
uses CONFIG_CONSOLE_VGA
uses CONFIG_VGA_ROM_RUN
uses CONFIG_PCI_ROM_RUN
uses DEBUG
# Toolchain
uses CC
uses HOSTCC
uses CROSS_COMPILE
uses OBJCOPY
# Tweaks
uses CONFIG_GDB_STUB
uses MAX_REBOOT_CNT
uses USE_WATCHDOG_ON_BOOT
uses COREBOOT_EXTRA_VERSION
uses MAINBOARD_POWER_ON_AFTER_POWER_FAIL

###
### Build options
###

##
##
default MAX_REBOOT_CNT=3

##
## Use the watchdog to break out of a lockup condition
##
default USE_WATCHDOG_ON_BOOT=0

##
## ROM_SIZE is the size of boot ROM that this board will use.
##
default ROM_SIZE=1024*1024


##
## Build code for the fallback boot
##
default HAVE_FALLBACK_BOOT=1

##
## Delay timer options
## Use timer2
## 
default CONFIG_UDELAY_TSC=1
default CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2=1

##
## Build code to reset the motherboard from coreboot
##
default HAVE_HARD_RESET=1

##
## Build SMI handler
##
default HAVE_SMI_HANDLER=1

##
## Leave a hole for mmapped PCIe config space
##

default CONFIG_PCIE_CONFIGSPACE_HOLE=1
default MMCONF_SUPPORT=1
default MMCONF_BASE_ADDRESS=0xf0000000

##
## UMA
##
default CONFIG_GFXUMA=1

##
## Build code to export a programmable irq routing table
##
default HAVE_PIRQ_TABLE=1
default IRQ_SLOT_COUNT=18

##
## Build code to export an x86 MP table
## Useful for specifying IRQ routing values
##
default HAVE_MP_TABLE=1

##
## Build code to provide ACPI support
##
default HAVE_ACPI_TABLES=1
default HAVE_MAINBOARD_RESOURCES=1
default HAVE_HIGH_TABLES=1

##
## Build code to export a CMOS option table
##
default HAVE_OPTION_TABLE=1

##
## Move the default coreboot cmos range off of AMD RTC registers
##
default LB_CKS_RANGE_START=49
default LB_CKS_RANGE_END=122
default LB_CKS_LOC=123

#VGA Console
default CONFIG_CONSOLE_VGA=1
# There are some network option roms that don't work with
# coreboot's x86emu. Thus, we only execute the VGA option rom
# for now:
default CONFIG_VGA_ROM_RUN=1
default CONFIG_PCI_ROM_RUN=0
default DEBUG=0

##
## Build code for SMP support
## Only worry about 2 micro processors
##
default CONFIG_SMP=1
default CONFIG_MAX_CPUS=4
default CONFIG_MAX_PHYSICAL_CPUS=2
default CONFIG_LOGICAL_CPUS=1
default CONFIG_AP_IN_SIPI_WAIT=1

##
## enable CACHE_AS_RAM specifics
##
default USE_DCACHE_RAM=1
default DCACHE_RAM_SIZE=0x8000
default DCACHE_RAM_BASE=( 0xfff00000 - DCACHE_RAM_SIZE - 1024*1024)
default CONFIG_USE_PRINTK_IN_CAR=1

##
## Build code to setup a generic IOAPIC
##
default CONFIG_IOAPIC=1

##
## Clean up the motherboard id strings
##
default MAINBOARD_PART_NUMBER="986LCD-M"
default MAINBOARD_VENDOR=     "KONTRON"

###
### coreboot layout values
###

## ROM_IMAGE_SIZE is the amount of space to allow coreboot to occupy.
default ROM_IMAGE_SIZE = 65536

##
## Use a small 8K stack
##
default STACK_SIZE=0x2000

##
## Use a small 32K heap
##
default HEAP_SIZE=0x8000


###
### Compute the location and size of where this firmware image
### (coreboot plus bootloader) will live in the boot rom chip.
###
default FALLBACK_SIZE=131072

##
## coreboot C code runs at this location in RAM
##
default _RAMBASE=0x00100000

##
## Load the payload from the ROM
##
default CONFIG_ROM_PAYLOAD=1

###
### Defaults of options that you may want to override in the target config file
### 

##
## The default compiler
##
default CC="$(CROSS_COMPILE)gcc -m32"
default HOSTCC="gcc"

##
## Disable the gdb stub by default
##
default CONFIG_GDB_STUB=0

##
## The Serial Console
##

# To Enable the Serial Console
default CONFIG_CONSOLE_SERIAL8250=1

## Select the serial console baud rate
default TTYS0_BAUD=115200
#default TTYS0_BAUD=57600
#default TTYS0_BAUD=38400
#default TTYS0_BAUD=19200
#default TTYS0_BAUD=9600
#default TTYS0_BAUD=4800
#default TTYS0_BAUD=2400
#default TTYS0_BAUD=1200

# Select the serial console base port
default TTYS0_BASE=0x3f8

# Select the serial protocol
# This defaults to 8 data bits, 1 stop bit, and no parity
default TTYS0_LCS=0x3

##
### Select the coreboot loglevel
##
## EMERG      1   system is unusable               
## ALERT      2   action must be taken immediately 
## CRIT       3   critical conditions              
## ERR        4   error conditions                 
## WARNING    5   warning conditions               
## NOTICE     6   normal but significant condition 
## INFO       7   informational                    
## DEBUG      8   debug-level messages             
## SPEW       9   Way too many details             

## Request this level of debugging output
default  DEFAULT_CONSOLE_LOGLEVEL=5
## At a maximum only compile in this level of debugging
default  MAXIMUM_CONSOLE_LOGLEVEL=9

##
## Select power on after power fail setting
default MAINBOARD_POWER_ON_AFTER_POWER_FAIL="MAINBOARD_POWER_ON"

#
# CBFS
# 
default CONFIG_CBFS=0

### End Options.lb
end
