##
## This file is part of the coreboot project.
##
## Copyright (C) 2008 VIA Technologies, Inc.
## (Written by Aaron Lwe <aaron.lwe@gmail.com> for VIA)
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

include /config/nofailovercalculation.lb

arch i386 end
driver mainboard.o
if HAVE_PIRQ_TABLE object irq_tables.o end
if HAVE_MP_TABLE object mptable.o end
if HAVE_ACPI_TABLES
	object fadt.o
	object dsdt.o
	object acpi_tables.o
end
makerule ./failover.E
	depends "$(MAINBOARD)/../../../arch/i386/lib/failover.c ../romcc"
	action "../romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/../../../arch/i386/lib/failover.c -o $@"
end
makerule ./failover.inc
	depends "$(MAINBOARD)/../../../arch/i386/lib/failover.c ../romcc"
	action "../romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/../../../arch/i386/lib/failover.c -o $@"
end
makerule ./auto.E
	depends	"$(MAINBOARD)/auto.c option_table.h ../romcc"
	action	"../romcc -E -mcpu=c3 -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc
	depends "$(MAINBOARD)/auto.c option_table.h ../romcc"
	action	"../romcc    -mcpu=c3 -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
ldscript /cpu/x86/32bit/entry32.lds
if USE_FALLBACK_IMAGE
	mainboardinit cpu/x86/16bit/reset16.inc
	ldscript /cpu/x86/16bit/reset16.lds
else
	mainboardinit cpu/x86/32bit/reset32.inc
	ldscript /cpu/x86/32bit/reset32.lds
end
mainboardinit arch/i386/lib/cpu_reset.inc
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds
if USE_FALLBACK_IMAGE
	ldscript /arch/i386/lib/failover.lds
	mainboardinit ./failover.inc
end
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc
dir /pc80
config chip.h

chip northbridge/via/cn700			# Northbridge
  device pci_domain 0 on			# PCI domain
    device pci 0.0 on end			# AGP Bridge
    device pci 0.1 on end			# Error Reporting
    device pci 0.2 on end			# Host Bus Control
    device pci 0.3 on end			# Memory Controller
    device pci 0.4 on end			# Power Management
    device pci 0.7 on end			# V-Link Controller
    device pci 1.0 on end			# PCI Bridge
    chip southbridge/via/vt8237r		# Southbridge
      # Enable both IDE channels.
      register "ide0_enable" = "1"
      register "ide1_enable" = "1"
      # Both cables are 40pin.
      register "ide0_80pin_cable" = "0"
      register "ide1_80pin_cable" = "0"
      register "fn_ctrl_lo" = "0x80"
      register "fn_ctrl_hi" = "0x1d"
      device pci f.0 on end			# IDE
      device pci 10.0 on end			# UHCI
      device pci 10.1 on end			# UHCI
      device pci 10.2 on end			# UHCI
      device pci 10.3 on end			# UHCI
      device pci 10.4 on end			# EHCI
      device pci 11.0 on			# Southbridge LPC
        chip superio/winbond/w83697hf		# Super I/O
          device pnp 2e.0 off			# Floppy
            io 0x60 = 0x3f0
            irq 0x70 = 6
            drq 0x74 = 2
          end
          device pnp 2e.1 on			# Parallel Port
            io 0x60 = 0x378
            irq 0x70 = 7
            drq 0x74 = 3
          end
          device pnp 2e.2 on			# COM1
            io 0x60 = 0x3f8
            irq 0x70 = 4
          end
          device pnp 2e.3 on			# COM2
            io 0x60 = 0x2f8
            irq 0x70 = 3
          end
          device pnp 2e.6 off end		# Consumer IR
          device pnp 2e.7 off end		# Game port, GPIO 1
          device pnp 2e.8 off end		# MIDI port, GPIO 5
          device pnp 2e.9 off end		# GPIO 2-4
          device pnp 2e.a off end		# ACPI
          device pnp 2e.b on			# HWM
            io 0x60 = 0x290
          end
        end
      end
      device pci 11.5 on end			# AC'97 audio
      device pci 12.0 on end			# Ethernet
    end
  end
  device apic_cluster 0 on			# APIC cluster
    chip cpu/via/model_c7			# VIA C7
      device apic 0 on end			# APIC
    end
  end
end
