target kontron_986lcd_m
mainboard kontron/986lcd-m

## ROM_SIZE is the total number of bytes allocated for coreboot use
## (normal AND fallback images and payloads).
option ROM_SIZE = 1024 * 1024

# Use this line instead if you want to use onboard VGA:
# option ROM_SIZE = (1024 * 1024) - (64 * 1024)

## ROM_IMAGE_SIZE is the maximum number of bytes allowed for a coreboot image,
## not including any payload.
option ROM_IMAGE_SIZE = 128 * 1024

## FALLBACK_SIZE is the amount of the ROM the complete fallback image 
## (including payload) will use.
option FALLBACK_SIZE = ROM_SIZE

romimage "fallback"
	option USE_FALLBACK_IMAGE=1
	payload ../payload.elf
end

buildrom ./coreboot.rom ROM_SIZE "fallback"
