##
## This file is part of the coreboot project.
##
## Copyright (C) 2006 AMD
## Written by Yinghai Lu <yinghailu@gmail.com> for AMD.
##
## Copyright (C) 2007 University of Mannheim
## Written by Philipp Degler <pdegler@rumms.uni-mannheim.e> for Uni of Mannheim
##
## Copyright (C) 2009 University of Heidelberg
## Written by Mondrian Nuessle <nuessle@uni-hd.de> for Uni of Heidelberg
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

include /config/nofailovercalculation.lb

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o

#needed by irq_tables and mptable and acpi_tables
object get_bus_conf.o

if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end

if CONFIG_USE_INIT
	makerule ./auto.o
		depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
		action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) -I$(TOP)/src -I. -c $(MAINBOARD)/cache_as_ram_auto.c -o $@"
	end
else
	makerule ./auto.inc
		depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
		action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) $(DEBUG_CFLAGS) -I$(TOP)/src -I. -c -S $(MAINBOARD)/cache_as_ram_auto.c -o $@"
		action "perl -e 's/\.rodata/.rom.data/g' -pi $@"
		action "perl -e 's/\.text/.section .rom.text/g' -pi $@"
	end
end

##
## Build our 16 bit and 32 bit coreboot entry code
##
if USE_FALLBACK_IMAGE
	mainboardinit cpu/x86/16bit/entry16.inc
	ldscript /cpu/x86/16bit/entry16.lds
end

mainboardinit cpu/x86/32bit/entry32.inc

	if CONFIG_USE_INIT
		ldscript /cpu/x86/32bit/entry32.lds
	end

	if CONFIG_USE_INIT
		ldscript /cpu/amd/car/cache_as_ram.lds
	end

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE
	mainboardinit cpu/x86/16bit/reset16.inc
	ldscript /cpu/x86/16bit/reset16.lds
else
	mainboardinit cpu/x86/32bit/reset32.inc
	ldscript /cpu/x86/32bit/reset32.lds
end

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

	##
	## Setup Cache-As-Ram
	##
	mainboardinit cpu/amd/car/cache_as_ram.inc

###
### This is the early phase of coreboot startup
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
		ldscript /arch/i386/lib/failover.lds
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
	if CONFIG_USE_INIT
		initobject auto.o
	else
		mainboardinit ./auto.inc
	end


# config for hp/dl145_g3
chip northbridge/amd/amdk8/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_F
			device apic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdk8  # northbridge
			device pci 18.0 on  # devices on link 0
				chip southbridge/broadcom/bcm21000 # HT2100
					device pci 0.0 on
					end   # bridge to slot PCI-E 4x ??
					device pci 1.0 on
					end
					device pci 2.0 on
					end  # unused
					device pci 3.0 on  	# bridge to slot PCI-E 16x ??
					end
					device pci 4.0 on
					end  # unused
					device pci 5.0 on
						device pci 4.0 on end # BCM5715 NIC
						device pci 4.1 on end # BCM5715 NIC
					end
				end
				chip southbridge/broadcom/bcm5785 # HT1000
					device pci 0.0 on  # HT PXB  0x0036
						device pci d.0 on end # PCI/PCI-X bridge 0x0104
						device pci e.0 on end # SATA 0x024a
					end
					device pci 1.0 on end # Legacy  pci main  0x0205
					device pci 1.1 on end # IDE	0x0214
					device pci 1.2 on     # LPC	0x0234
						chip superio/nsc/pc87417
							device  pnp 4e.0 off  # Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 4e.1 off  # Parallel Port
									io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 4e.2 off # Com 2
									io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 4e.3 off  # Com 1
									io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 4e.4 off end # SWC
							device pnp 4e.5 off end # Mouse
							device pnp 4e.6 off  # Keyboard
									io 0x60 = 0x60
									io 0x62 = 0x64
								irq 0x70 = 1
							end
							device pnp 4e.7 off end # GPIO
							device pnp 4e.f off end # XBUS
							device pnp 4e.10 on #RTC
								io 0x60 = 0x70
								io 0x62 = 0x72
							end
						end # end superio
					end # end pci 1.2
					device pci 1.3 off end # WDTimer    0x0238
					device pci 1.4 on end # XIOAPIC0   0x0235
					device pci 1.5 on end # XIOAPIC1
					device pci 1.6 on end # XIOAPIC2
					device pci 2.0 on end # USB	0x0223
					device pci 2.1 on end # USB
					device pci 2.2 on end # USB
 					chip drivers/pci/onboard
						# it is in bcm5785_0 bus, but the device id can
						# not be changed even unitid is changed, fake one
						# to get the rom_address
						# if HT_CHAIN_END_UNITID_BASE=0, it is 4,
						# if HT_CHAIN_END_UNITID_BASE=1, it is 3
 						device pci 4.0 on end
 						register "rom_address" = "0xfff00000"
 					end
					#bx_a013+ start
					#chip drivers/pci/onboard    #SATA2
					#	device pci 5.0 on end
					#	device pci 5.1 on end
					#	device pci 5.2 on end
					#	device pci 5.3 on end
					#end
					#bx_a013+ end
				end
			end
			device pci 18.0 on end
			device pci 18.0 on end
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
      end # amdk8

   end #pci_domain
end


