include /config/nofailovercalculation.lb

##
## Set all of the defaults for an x86 architecture
##

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o
if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
#object reset.o

if CONFIG_USE_INIT

makerule ./auto.o
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) -I$(TOP)/src -I. -c $(MAINBOARD)/cache_as_ram_auto.c -o $@"
end

else    
                
makerule ./auto.inc
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) $(DEBUG_CFLAGS) -I$(TOP)/src -I. -c -S $(MAINBOARD)/cache_as_ram_auto.c -o $@"
        action "perl -e 's/\.rodata/.rom.data/g' -pi $@"
        action "perl -e 's/\.text/.section .rom.text/g' -pi $@"
end

end

##
## Build our 16 bit and 32 bit coreboot entry code
##
if USE_FALLBACK_IMAGE
        mainboardinit cpu/x86/16bit/entry16.inc
        ldscript /cpu/x86/16bit/entry16.lds
end

mainboardinit cpu/x86/32bit/entry32.inc

        if CONFIG_USE_INIT
                ldscript /cpu/x86/32bit/entry32.lds
        end

        if CONFIG_USE_INIT
                ldscript      /cpu/amd/car/cache_as_ram.lds
        end

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

##
## Setup Cache-As-Ram
##
mainboardinit cpu/amd/car/cache_as_ram.inc

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
       ldscript /arch/i386/lib/failover.lds
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
if CONFIG_USE_INIT
initobject auto.o
else
mainboardinit ./auto.inc
end

##
## Include the secondary Configuration files 
##
config chip.h


chip northbridge/amd/amdk8/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_940
			device apic 0 on end
		end
	end

	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on end # LDT 0
			device pci 18.0 on     # LDT 1
				chip southbridge/amd/amd8131
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
                                                chip drivers/pci/onboard
                                                        device pci 5.0 on end # ATI Rage XL
                                                        register "rom_address" = "0xfff80000"
                                                end
					end
					device pci 1.0 on
						chip superio/nsc/pc87366
							device	pnp 2e.0 off  # Floppy 
								 io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off  # Parallel Port
								 io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 off # Com 2
								 io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.3 on  # Com 1
								 io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.4 off end # SWC
							device pnp 2e.5 off end # Mouse
							device pnp 2e.6 on  # Keyboard
								 io 0x60 = 0x60
								 io 0x62 = 0x64
								irq 0x70 = 1
							end
							device pnp 2e.7 off end # GPIO
							device pnp 2e.8 off end # ACB
							device pnp 2e.9 off end # FSCM
							device pnp 2e.a off end # WDT  
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 off end
					device pci 1.6 off end
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
				end
			end #  device pci 18.0 
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end 
end

