include /config/nofailovercalculation.lb

##
## Set all of the defaults for an x86 architecture
##

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o
if HAVE_PIRQ_TABLE object irq_tables.o end
#object reset.o
object vgabios.o

if HAVE_ACPI_TABLES
	object fadt.o
	object dsdt.o
	object acpi_tables.o
end

##
## Romcc output
##
makerule ./failover.E
	depends "$(MAINBOARD)/failover.c ../romcc" 
	action "../romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./failover.inc
	depends "$(MAINBOARD)/failover.c ../romcc"
	action "../romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./auto.E 
	depends	"$(MAINBOARD)/auto.c option_table.h ../romcc" 
	action	"../romcc -E -mcpu=c3 -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc 
	depends "$(MAINBOARD)/auto.c option_table.h ../romcc"
	action	"../romcc    -mcpu=c3 -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end

##
## Build our 16 bit and 32 bit coreboot entry code
##
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
ldscript /cpu/x86/32bit/entry32.lds

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

### Should this be in the northbridge code?
mainboardinit arch/i386/lib/cpu_reset.inc

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
	ldscript /arch/i386/lib/failover.lds 
	mainboardinit ./failover.inc
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc

##
## Include the secondary Configuration files 
##
dir /pc80
config chip.h

chip northbridge/via/vt8623

	device apic_cluster 0 on
		chip cpu/via/model_c3
			device apic 0 on  end 
		end
	end

	device pci_domain 0 on
		chip southbridge/via/vt8235

			device pci 10.0 on end # USB 1.1
			device pci 10.1 on end # USB 1.1
			device pci 10.2 on end # USB 1.1
			device pci 10.3 on end # USB 2

			device pci 11.0 on      # Southbridge
				chip superio/via/vt1211
					device pnp 2e.0 on	# Floppy
						io 0x60 = 0x3f0
						irq 0x70 = 6
						drq 0x74 = 2
					end
					device pnp 2e.1 on	# Parallel Port
						io 0x60 = 0x378
						irq 0x70 = 7
						drq 0x74 = 3
					end
					device pnp 2e.2 on	# COM1
						io 0x60 = 0x3f8
						irq 0x70 = 4
					end
					device pnp 2e.3 on	# COM2
						io 0x60 = 0x2f8
						irq 0x70 = 3
					end
					device pnp 2e.b on	# HWM
						io 0x60 = 0xec00
					end

				end
			end
			
			device pci 11.1 on  end # IDE
			# 2-4 non existant?
			device pci 11.5 on  end # AC97 Audio
			device pci 11.6 off end # AC97 Modem
			device pci 12.0 on end  # Ethernet
		end
#		This is on the EPIA MII, not the M.
		chip southbridge/ricoh/rl5c476
			register "enable_cf" = "1"
			device pci 0a.0 on end
			device pci 0a.1 on end	
		end
	end
end
