#
# This file is part of the coreboot project.
#
# Copyright (C) 2007 Advanced Micro Devices, Inc.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License as published by
# the Free Software Foundation; version 2 of the License.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.	 See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
#

include /config/failovercalculation.lb

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o


#needed by irq_tables and mptable and acpi_tables
object get_bus_conf.o

if HAVE_MP_TABLE
	object mptable.o
end

if HAVE_PIRQ_TABLE
	object irq_tables.o
end

if HAVE_ACPI_TABLES
	 object acpi_tables.o
	 object fadt.o
	makerule dsdt.c
		depends "$(MAINBOARD)/dx/dsdt_lb.dsl"
		action	"iasl -p $(PWD)/dsdt_lb -tc $(MAINBOARD)/dx/dsdt_lb.dsl"
		action	"mv dsdt_lb.hex dsdt.c"
	end
	 object ./dsdt.o

	#./ssdt.o is moved to northbridge/amd/amdk8/Config.lb

	if ACPI_SSDTX_NUM
	makerule ssdt2.c
		depends "$(MAINBOARD)/dx/pci2.asl"
		action	"iasl -p $(PWD)/pci2 -tc $(MAINBOARD)/dx/pci2.asl"
		action	"perl -pi -e 's/AmlCode/AmlCode_ssdt2/g' pci2.hex"
		action	"mv pci2.hex ssdt2.c"
	end
	object ./ssdt2.o
	makerule ssdt3.c
		depends "$(MAINBOARD)/dx/pci3.asl"
		action	"iasl -p $(PWD)/pci3 -tc $(MAINBOARD)/dx/pci3.asl"
		action	"perl -pi -e 's/AmlCode/AmlCode_ssdt3/g' pci3.hex"
		action	"mv pci3.hex ssdt3.c"
	end
	object ./ssdt3.o
	makerule ssdt4.c
		depends "$(MAINBOARD)/dx/pci4.asl"
		action	"iasl -p $(PWD)/pci4 -tc $(MAINBOARD)/dx/pci4.asl"
		action	"perl -pi -e 's/AmlCode/AmlCode_ssdt4/g' pci4.hex"
		action	"mv pci4.hex ssdt4.c"
	end
	object ./ssdt4.o
	makerule ssdt5.c
		depends "$(MAINBOARD)/dx/pci5.asl"
		action	"iasl -p $(PWD)/pci5 -tc $(MAINBOARD)/dx/pci5.asl"
		action	"perl -pi -e 's/AmlCode/AmlCode_ssdt5/g' pci5.hex"
		action	"mv pci5.hex ssdt5.c"
	end
	object ./ssdt5.o
	 end
end

	if CONFIG_USE_INIT
		# compile cache_as_ram.c to auto.o
		makerule ./cache_as_ram_auto.o
			depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
			action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) -I$(TOP)/src -I. -c $(MAINBOARD)/cache_as_ram_auto.c -o $@"
		end

	else
		#compile cache_as_ram.c to auto.inc
		makerule ./cache_as_ram_auto.inc
			depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
			action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) $(DEBUG_CFLAGS) -I$(TOP)/src -I. -c -S $(MAINBOARD)/cache_as_ram_auto.c -o $@"
			action "perl -e 's/\.rodata/.rom.data/g' -pi $@"
			action "perl -e 's/\.text/.section .rom.text/g' -pi $@"
		end

	end

if USE_FAILOVER_IMAGE
else
    if CONFIG_AP_CODE_IN_CAR
	 makerule ./apc_auto.o
		 depends "$(MAINBOARD)/apc_auto.c option_table.h"
		 action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) -I$(TOP)/src -I. -c $(MAINBOARD)/apc_auto.c -o $@"
	 end
	 ldscript /arch/i386/init/ldscript_apc.lb
    end
end

##
## Build our 16 bit and 32 bit coreboot entry code
##

if HAVE_FAILOVER_BOOT
    if USE_FAILOVER_IMAGE
	mainboardinit cpu/x86/16bit/entry16.inc
	ldscript /cpu/x86/16bit/entry16.lds
    end
else
    if USE_FALLBACK_IMAGE
	mainboardinit cpu/x86/16bit/entry16.inc
	ldscript /cpu/x86/16bit/entry16.lds
    end
end

mainboardinit cpu/x86/32bit/entry32.inc
	 if CONFIG_USE_INIT
		 ldscript /cpu/x86/32bit/entry32.lds
	 end

	 if CONFIG_USE_INIT
		 ldscript /cpu/amd/car/cache_as_ram.lds
	 end

##
## Build our reset vector (This is where coreboot is entered)
##
if HAVE_FAILOVER_BOOT
    if USE_FAILOVER_IMAGE
	mainboardinit cpu/x86/16bit/reset16.inc
	ldscript /cpu/x86/16bit/reset16.lds
    else
	mainboardinit cpu/x86/32bit/reset32.inc
	ldscript /cpu/x86/32bit/reset32.lds
    end
else
    if USE_FALLBACK_IMAGE
	mainboardinit cpu/x86/16bit/reset16.inc
	ldscript /cpu/x86/16bit/reset16.lds
    else
	mainboardinit cpu/x86/32bit/reset32.inc
	ldscript /cpu/x86/32bit/reset32.lds
    end
end


##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

	##
	## Setup Cache-As-Ram
	##
	mainboardinit cpu/amd/car/cache_as_ram.inc

###
### This is the early phase of coreboot startup
### Things are delicate and we test to see if we should
### failover to another image.
###
if HAVE_FAILOVER_BOOT
    if USE_FAILOVER_IMAGE
		ldscript /arch/i386/lib/failover_failover.lds
    end
else
    if USE_FALLBACK_IMAGE
		ldscript /arch/i386/lib/failover.lds
    end
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
	if CONFIG_USE_INIT
		initobject cache_as_ram_auto.o
	else
		mainboardinit ./cache_as_ram_auto.inc
	end

##
## Include the secondary Configuration files
##
config chip.h

dir /southbridge/amd/amd8151

# sample config for amd/serengeti_cheetah_fam10
chip northbridge/amd/amdfam10/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_F_1207  #L1 and DDR2
			 device apic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdfam10
			device pci 18.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/amd/amd8132
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 off end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 off #  Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off #  Parallel Port
								io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 on #  Com1
								io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.3 off #  Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.5 on #  Keyboard
								io 0x60 = 0x60
								io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.6 off #  CIR
								io 0x60 = 0x100
							end
							device pnp 2e.7 off #  GAME_MIDI_GIPO1
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end
							device pnp 2e.8 off end #  GPIO2
							device pnp 2e.9 off end #  GPIO3
							device pnp 2e.a off end #  ACPI
							device pnp 2e.b on #  HW Monitor
								io 0x60 = 0x290
								irq 0x70 = 5
							end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on
						chip drivers/i2c/i2cmux2 # pca9556 smbus mux
						chip drivers/i2c/i2cmux2 # pca9556 smbus mux
							device i2c 18 on #0 pca9516 1
								chip drivers/generic/generic #dimm 0-0-0
									device i2c 50 on end
								end
								chip drivers/generic/generic #dimm 0-0-1
									device i2c 51 on end
								end
								chip drivers/generic/generic #dimm 0-1-0
									device i2c 52 on end
								end
								chip drivers/generic/generic #dimm 0-1-1
									device i2c 53 on end
								end
							end
							device i2c 18 on #1 pca9516 2
								chip drivers/generic/generic #dimm 1-0-0
									device i2c 50 on end
								end
								chip drivers/generic/generic #dimm 1-0-1
									device i2c 51 on end
								end
								chip drivers/generic/generic #dimm 1-1-0
									device i2c 52 on end
								end
								chip drivers/generic/generic #dimm 1-1-1
									device i2c 53 on end
								end
							end
						end
						end
					end # acpi
					device pci 1.5 off end
					device pci 1.6 off end
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
				end
			end #  device pci 18.0

			device pci 18.0 on end
			device pci 18.0 on end
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
			device pci 18.4 on end
#			device pci 00.5 on end
		end
	end #pci_domain
	#for node 32 to node 63
#	device pci_domain 0 on
#		chip northbridge/amd/amdfam10
#			  device pci 00.0 on end#  northbridge
#			  device pci 00.0 on end
#			  device pci 00.0 on end
#			  device pci 00.0 on end
#			  device pci 00.1 on end
#			  device pci 00.2 on end
#			  device pci 00.3 on end
#			  device pci 00.4 on end
#			 device pci 00.5 on end
#		end
#	end #pci_domain

#	  chip drivers/generic/debug
#		 device pnp 0.0 off end # chip name
#		  device pnp 0.1 on end # pci_regs_all
#		  device pnp 0.2 off end # mem
#		  device pnp 0.3 off end # cpuid
#		  device pnp 0.4 off end # smbus_regs_all
#		  device pnp 0.5 off end # dual core msr
#		  device pnp 0.6 off end # cache size
#		  device pnp 0.7 off end # tsc
#		  device pnp 0.8 off end # hard reset
#		  device pnp 0.9 off end # mcp55
#		  device pnp 0.a on end # GH ext table
#	 end

end


