##
## Only use the option table in a normal image
##
default USE_OPTION_TABLE = !USE_FALLBACK_IMAGE

include /config/nofailovercalculation128.lb

## Set all of the defaults for an x86 architecture
##

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o
if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
object reset.o

##
## Romcc output
##
makerule ./failover.E
	depends "$(MAINBOARD)/failover.c ../romcc"
	action "../romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./failover.inc
	depends "$(MAINBOARD)/failover.c ../romcc"
	action "../romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./auto.E 
	depends	"$(MAINBOARD)/auto.c option_table.h ../romcc" 
	action	"../romcc -E -mcpu=p4 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end

makerule ./auto.inc 
	depends	"$(MAINBOARD)/auto.c option_table.h ../romcc" 
	action	"../romcc    -mcpu=p4 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end

##
## Build our 16 bit and 32 bit coreboot entry code
##
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
ldscript /cpu/x86/32bit/entry32.lds

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

### Should this be in the northbridge code?
mainboardinit arch/i386/lib/cpu_reset.inc

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
	ldscript /arch/i386/lib/failover.lds 
	mainboardinit ./failover.inc
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit cpu/x86/sse/enable_sse.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/sse/disable_sse.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc


##
## Include the secondary Configuration files 
##
dir /pc80
config chip.h

chip northbridge/intel/e7520  # MCH
	chip drivers/generic/debug  # DEBUGGING
		device pnp 00.0 on end
		device pnp 00.1 off end
		device pnp 00.2 off end
		device pnp 00.3 off end
	end
	device pci_domain 0 on
		chip southbridge/intel/esb6300	# ESB6300
			register "pirq_a_d" = "0x0b070a05"
			register "pirq_e_h" = "0x0a808080"

			device pci 1c.0 on 
				chip drivers/generic/generic 
					device pci 01.0 on end	# onboard gige1
					device pci 02.0 on end 	# onboard gige2
				end
			end

			# USB ports
			device pci 1d.0 on end
			device pci 1d.1 on end
			device pci 1d.4 on end	# Southbridge Watchdog timer
			device pci 1d.5 on end	# Southbridge I/O apic1
			device pci 1d.7 on end

			# VGA / PCI 32-bit
			device pci 1e.0 on 
				chip drivers/generic/generic
					device pci 01.0 on end 
				end
			end


			device pci 1f.0 on 	# ISA bridge
				chip superio/winbond/w83627hf
					device pnp 2e.0 off end
					device pnp 2e.2 on 
						 io 0x60 = 0x3f8
						irq 0x70 = 4
					end
					device pnp 2e.3 on
						 io 0x60 = 0x2f8
						irq 0x70 = 3
					end
					device pnp 2e.4 off end
					device pnp 2e.5 off end
					device pnp 2e.6 off end
					device pnp 2e.7 off end
					device pnp 2e.9 off end
					device pnp 2e.a on end
					device pnp 2e.b off end
				end
			end
			device pci 1f.1 on end
			device pci 1f.2 off end
			device pci 1f.3	on end		# SMBus
			device pci 1f.5 off end
			device pci 1f.6 off end
		end

		device pci 00.0	on end	# Northbridge
		device pci 00.1	on end  # Northbridge Error reporting
		device pci 01.0 on end
		device pci 02.0 on 
			chip southbridge/intel/pxhd	# PXHD 6700 
				device pci 00.0 on end   # bridge 
				device pci 00.1 on end   # I/O apic
				device pci 00.2 on end   # bridge
				device pci 00.3 on end   # I/O apic
			end
		end
#	 	device register "intrline" = "0x00070105" 
		device 	pci 04.0 on end	
		device 	pci 06.0 on end	
	end

	device apic_cluster 0 on
		chip cpu/intel/socket_mPGA604  	# CPU 0
			device apic 0 on end
		end
		chip cpu/intel/socket_mPGA604 	# CPU 1
			device apic 6 on end
		end
	end
end
