include /config/nofailovercalculation.lb

##
## Set all of the defaults for an x86 architecture
##

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o
if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
#object reset.o

if CONFIG_USE_INIT

makerule ./auto.o
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) -I$(TOP)/src -I. -c $(MAINBOARD)/cache_as_ram_auto.c -o $@"
end

else    
                
makerule ./auto.inc
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) $(DISTRO_CFLAGS) $(CFLAGS) $(CPPFLAGS) $(DEBUG_CFLAGS) -I$(TOP)/src -I. -c -S $(MAINBOARD)/cache_as_ram_auto.c -o $@"
        action "perl -e 's/\.rodata/.rom.data/g' -pi $@"
        action "perl -e 's/\.text/.section .rom.text/g' -pi $@"
end

end

##
## Build our 16 bit and 32 bit coreboot entry code
##
if USE_FALLBACK_IMAGE
        mainboardinit cpu/x86/16bit/entry16.inc
        ldscript /cpu/x86/16bit/entry16.lds
end

mainboardinit cpu/x86/32bit/entry32.inc

        if CONFIG_USE_INIT
                ldscript /cpu/x86/32bit/entry32.lds
        end

        if CONFIG_USE_INIT
                ldscript      /cpu/amd/car/cache_as_ram.lds
        end

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

##
## Setup Cache-As-Ram
##
mainboardinit cpu/amd/car/cache_as_ram.inc

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
       ldscript /arch/i386/lib/failover.lds
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
if CONFIG_USE_INIT
initobject auto.o
else
mainboardinit ./auto.inc
end

##
## Include the secondary Configuration files 
##
config chip.h

chip northbridge/amd/amdk8/root_complex
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge 
				#  devices on link 0, link 0 == LDT 0 
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/winbond/w83627thf
							device pnp 2e.0 on end
							device pnp 2e.1 on end
							device pnp 2e.2 on end
							device pnp 2e.3 on end
							device pnp 2e.4 on end
							device pnp 2e.5 on end
							device pnp 2e.6 on end
							device pnp 2e.7 on end 
							device pnp 2e.8 on end 
							device pnp 2e.9 on end 
							device pnp 2e.a on end 
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end 
					device pci 1.5 off end
					device pci 1.6 off end
				end
			end # LDT0
			device pci 18.0 on end # LDT1
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
		chip northbridge/amd/amdk8
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.1 on end
			device pci 19.2 on end
			device pci 19.3 on end
		end
	end 
	device apic_cluster 0 on
		chip cpu/amd/socket_940
			device apic 0 on end
		end
		chip cpu/amd/socket_940
			device apic 1 on end
		end
	end
end

