##
## This file is part of the coreboot project.
##
## Copyright (C) 2008 LiPPERT Embedded Computers GmbH
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

# Config file for the LiPPERT Cool RoadRunner-LX,		--JR 10/2008
# based on Config.lb for the AMD Geode LX/5536 DB800 platform.

target roadrunner-lx
mainboard lippert/roadrunner-lx

# HACK to get the right TSC support.
option CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2 = 1

option CONFIG_COMPRESSED_PAYLOAD_NRV2B = 0
option CONFIG_COMPRESSED_PAYLOAD_LZMA = 0

## Load payload (e.g. Linux) from IDE.
#option CONFIG_ROM_PAYLOAD = 0
#option CONFIG_IDE = 1
#option CONFIG_FS_PAYLOAD = 1
#option CONFIG_FS_EXT2 = 1
#option AUTOBOOT_DELAY = 0
#option AUTOBOOT_CMDLINE = "hda1:/payload.elf"

# Leave 36k for VSA. Usually board is equipped with a 512 KB FWH (LPC) flash,
# however it can be replaced with a 1 MB chip.
option ROM_SIZE = (512 * 1024) - (36 * 1024)
#option ROM_SIZE = (1024 * 1024) - (36 * 1024)
option FALLBACK_SIZE = ROM_SIZE

#option DEFAULT_CONSOLE_LOGLEVEL = 4
#option MAXIMUM_CONSOLE_LOGLEVEL = 4

# Saves space on ROM_IMAGE_SIZE, but decompression costs a second on boot.
option CONFIG_COMPRESS = 1

romimage "image"
	option USE_FALLBACK_IMAGE = 1
	option ROM_IMAGE_SIZE = 64 * 1024
	option COREBOOT_EXTRA_VERSION = ".0"
	payload ../payload.elf
	# If getting payload from IDE
	# payload /dev/null
end

buildrom ./coreboot.rom ROM_SIZE "image"
