chip northbridge/amd/amdfam10/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_F_1207  #L1 and DDR2
			 device apic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdfam10
			device pci 18.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/amd/amd8132
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 off end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 off #  Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off #  Parallel Port
								io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 on #  Com1
								io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.3 off #  Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.5 on #  Keyboard
								io 0x60 = 0x60
								io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.6 off #  CIR
								io 0x60 = 0x100
							end
							device pnp 2e.7 off #  GAME_MIDI_GIPO1
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end
							device pnp 2e.8 off end #  GPIO2
							device pnp 2e.9 off end #  GPIO3
							device pnp 2e.a off end #  ACPI
							device pnp 2e.b on #  HW Monitor
								io 0x60 = 0x290
								irq 0x70 = 5
							end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on
						chip drivers/i2c/i2cmux2 # pca9556 smbus mux
						chip drivers/i2c/i2cmux2 # pca9556 smbus mux
							device i2c 18 on #0 pca9516 1
								chip drivers/generic/generic #dimm 0-0-0
									device i2c 50 on end
								end
								chip drivers/generic/generic #dimm 0-0-1
									device i2c 51 on end
								end
								chip drivers/generic/generic #dimm 0-1-0
									device i2c 52 on end
								end
								chip drivers/generic/generic #dimm 0-1-1
									device i2c 53 on end
								end
							end
							device i2c 18 on #1 pca9516 2
								chip drivers/generic/generic #dimm 1-0-0
									device i2c 50 on end
								end
								chip drivers/generic/generic #dimm 1-0-1
									device i2c 51 on end
								end
								chip drivers/generic/generic #dimm 1-1-0
									device i2c 52 on end
								end
								chip drivers/generic/generic #dimm 1-1-1
									device i2c 53 on end
								end
							end
						end
						end
					end # acpi
					device pci 1.5 off end
					device pci 1.6 off end
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
				end
			end #  device pci 18.0

			device pci 18.0 on end
			device pci 18.0 on end
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
			device pci 18.4 on end
#			device pci 00.5 on end
		end
	end #pci_domain
	#for node 32 to node 63
#	device pci_domain 0 on
#		chip northbridge/amd/amdfam10
#			  device pci 00.0 on end#  northbridge
#			  device pci 00.0 on end
#			  device pci 00.0 on end
#			  device pci 00.0 on end
#			  device pci 00.1 on end
#			  device pci 00.2 on end
#			  device pci 00.3 on end
#			  device pci 00.4 on end
#			 device pci 00.5 on end
#		end
#	end #pci_domain

#	  chip drivers/generic/debug
#		 device pnp 0.0 off end # chip name
#		  device pnp 0.1 on end # pci_regs_all
#		  device pnp 0.2 off end # mem
#		  device pnp 0.3 off end # cpuid
#		  device pnp 0.4 off end # smbus_regs_all
#		  device pnp 0.5 off end # dual core msr
#		  device pnp 0.6 off end # cache size
#		  device pnp 0.7 off end # tsc
#		  device pnp 0.8 off end # hard reset
#		  device pnp 0.9 off end # mcp55
#		  device pnp 0.a on end # GH ext table
#	 end

end


