chip northbridge/amd/amdk8/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_F
                        device apic 0 on end
                end
        end
	device pci_domain 0 on
		chip northbridge/amd/amdk8 #mc0
			device pci 18.0 on end
			device pci 18.0 on end
			device pci 18.0 on 
				#  devices on link 0, link 0 == LDT 0 
			        chip southbridge/nvidia/mcp55 
					device pci 0.0 on end   # HT
                			device pci 1.0 on # LPC
						chip superio/winbond/w83627hf
							device pnp 2e.0 off #  Floppy
                	                 			io 0x60 = 0x3f0
                	                			irq 0x70 = 6
                	                			drq 0x74 = 2
							end
                	        			device pnp 2e.1 off #  Parallel Port
                	                 			io 0x60 = 0x378
                	                			irq 0x70 = 7
							end
                	        			device pnp 2e.2 on #  Com1
                	                 			io 0x60 = 0x3f8
                	                			irq 0x70 = 4
							end
                	        			device pnp 2e.3 off #  Com2
                	                 			io 0x60 = 0x2f8
                	                			irq 0x70 = 3
							end
                	        			device pnp 2e.5 on #  Keyboard
                	                 			io 0x60 = 0x60
                	                 			io 0x62 = 0x64
                	                			irq 0x70 = 1
								irq 0x72 = 12
							end
                	        			device pnp 2e.6 off  # SFI 
                	                 			io 0x62 = 0x100
							end
                	        			device pnp 2e.7 off #  GPIO_GAME_MIDI
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end						
                	        			device pnp 2e.8 off end #  WDTO_PLED
                	        			device pnp 2e.9 off end #  GPIO_SUSLED
                	        			device pnp 2e.a off end #  ACPI
                	        			device pnp 2e.b on #  HW Monitor
 					 			io 0x60 = 0x290
								irq 0x70 = 5
                					end
						end
					end
			                device pci 1.1 on # SM 0
						chip drivers/i2c/i2cmux2
							device i2c 48 off end
							device i2c 49 off end
						end
					end # SM
                                        device pci 1.1 on # SM 1
#PCI device smbus address will depend on addon pci device, do we need to scan_smbus_bus?
#                                                chip drivers/generic/generic #PCIXA Slot1
#                                                        device i2c 50 on end
#                                                end
#                                                chip drivers/generic/generic #PCIXB Slot1
#                                                        device i2c 51 on end
#                                                end     
#                                                chip drivers/generic/generic #PCIXB Slot2
#                                                        device i2c 52 on end
#                                                end             
#                                                chip drivers/generic/generic #PCI Slot1
#                                                        device i2c 53 on end
#                                                end              
#                                                chip drivers/generic/generic #Master MCP55 PCI-E
#                                                        device i2c 54 on end
#                                                end     
#                                                chip drivers/generic/generic #Slave MCP55 PCI-E
#                                                        device i2c 55 on end
#                                                end             
                                                chip drivers/generic/generic #MAC EEPROM
                                                        device i2c 51 on end
                                                end

                                        end # SM 
	                		device pci 2.0 on end # USB 1.1
        	        		device pci 2.1 on end # USB 2
                			device pci 4.0 on end # IDE
	                		device pci 5.0 on end # SATA 0
	                		device pci 5.1 on end # SATA 1
	                		device pci 5.2 on end # SATA 2
                			device pci 6.0 on  # PCI
                                                device pci 6.0 on end
					end
        	        		device pci 6.1 on end # AZA
	                		device pci 8.0 on end # NIC
	                		device pci 9.0 on end # NIC
        	       			device pci a.0 on  # PCI E 5
						device pci 0.0 on #nec pci-x
						end
						device pci 0.1 on #nec pci-x
							device pci 4.0 on end #scsi
							device pci 4.1 on end #scsi
						end
					end
        	       			device pci b.0 on end # PCI E 4
                			device pci c.0 on end # PCI E 3
                			device pci d.0 on end # PCI E 2
                			device pci e.0 on end # PCI E 1
        	       			device pci f.0 on end # PCI E 0
	                                register "ide0_enable" = "1"
                	                register "sata0_enable" = "1"
                        	        register "sata1_enable" = "1"
					register "mac_eeprom_smbus" = "3" # 1: smbus under 2e.8, 2: SM0 3: SM1
					register "mac_eeprom_addr" = "0x51"
				end
			end #  device pci 18.0 
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end # mc0
		
	end # PCI domain
	
#       chip drivers/generic/debug 
#               device pnp 0.0 off end # chip name
#                device pnp 0.1 on end # pci_regs_all
#                device pnp 0.2 off end # mem
#                device pnp 0.3 off end # cpuid
#                device pnp 0.4 on end # smbus_regs_all
#                device pnp 0.5 off end # dual core msr
#                device pnp 0.6 off end # cache size
#                device pnp 0.7 off end # tsc
#                device pnp 0.8 off  end # io
#                device pnp 0.9 on end # io
#       end  
end #root_complex
