chip northbridge/amd/gx1
  device pci_domain 0 on
    device pci 0.0 on end
      chip southbridge/amd/cs5530
        device pci 0a.0 on  end		# ETH0
        device pci 0b.0 off end		# ETH1
        device pci 0c.0 on  end		# ETH2
        device pci 0f.0 on  end		# PCI slot
        device pci 12.0 on
          chip superio/winbond/w83977tf
            device pnp 2e.0 on		# FDC
              irq 0x70 = 6
            end
            device pnp 2e.1 on		# Parallel Port
               io 0x60 = 0x378
              irq 0x70 = 7
            end
            device pnp 2e.2 on		# COM1
               io 0x60 = 0x3f8
              irq 0x70 = 4
            end
            register "com1" = "{115200}"
            device pnp 2e.3 on		# COM2
               io 0x60 = 0x2f8
              irq 0x70 = 3
            end
            register "com2" = "{115200}"
            device pnp 2e.4 off		# Reserved
            end
            device pnp 2e.5 on		# Keyboard
               io 0x60 = 0x60
               io 0x62 = 0x64
              irq 0x70 = 0x01		# Int  1 for PS/2 keyboard
              irq 0x72 = 0x0c		# Int 12 for PS/2 mouse
            end
            device pnp 2e.6 on		# IR
               io 0x60 = 0x2e8
              irq 0x70 = 3
            end
            device pnp 2e.7 on		# GAME/MIDI/GPIO1
               io 0x60 = 0x290
            end
            device pnp 2e.8 on		# GPIO2
               io 0x60 = 0x110
            end
            device pnp 2e.9 on		# GPIO3
               io 0x60 = 0x120
            end
            device pnp 2e.A on		# Power Management
               io 0x60 = 0xe800
            end
          end
        device pci 12.1 on  end		# SMI
        device pci 12.2 on  end		# IDE
        device pci 12.3 on  end		# Audio
        device pci 12.4 on  end		# VGA onboard
      end
      device pci 13.0 on end		# USB
    end
  end

  chip cpu/amd/model_gx1
  end

end

