chip northbridge/amd/amdk8/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_940
			device apic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdk8 #mc0
			device pci 18.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/nvidia/ck804
					device pci 0.0 on end   # HT
					device pci 1.0 on # LPC
						chip superio/smsc/lpc47b397
							device pnp 2e.0 on #  Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.3 on #  Parallel Port
								io 0x60 = 0x378
								irq 0x70 = 7
								drq 0x74 = 4
							end
							device pnp 2e.4 on #  Com1
								io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.5 off #  Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.7 on #  Keyboard
								io 0x60 = 0x60
								io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.8 on # HW Monitor
								io 0x60 = 0x480
								chip drivers/generic/generic # LM95221 CPU temp
									device i2c 2b on end
								end
								chip drivers/generic/generic # EMCT03
									device i2c 54 on end
								end
							end
							device	pnp 2e.a on #  RT
								io 0x60 = 0x400
							end
						end
					end
					device pci 1.1 on # SM 0
						chip drivers/generic/generic #dimm 0-0-0
							device i2c 50 on end
						end
						chip drivers/generic/generic #dimm 0-0-1
							device i2c 51 on end
						end
						chip drivers/generic/generic #dimm 0-1-0
							device i2c 52 on end
						end
						chip drivers/generic/generic #dimm 0-1-1
							device i2c 53 on end
						end
						chip drivers/generic/generic #dimm 1-0-0
							device i2c 54 on end
						end
						chip drivers/generic/generic #dimm 1-0-1
							device i2c 55 on end
						end
						chip drivers/generic/generic #dimm 1-1-0
							device i2c 56 on end
						end
						chip drivers/generic/generic #dimm 1-1-1
							device i2c 57 on end
						end
					end # SM
					device pci 1.1 on # SM 1
						chip drivers/generic/generic #MAC EEPROM
							device i2c 51 on end
						end

					end # SM
					device pci 2.0 on end # USB 1.1
					device pci 2.1 on end # USB 2
					device pci 4.0 on end # ACI
					device pci 4.1 off end # MCI
					device pci 6.0 on end # IDE
					device pci 7.0 on end # SATA 1
					device pci 8.0 on end # SATA 0
					device pci 9.0 on end # PCI
					device pci a.0 on end # NIC
					device pci b.0 off end # PCI E 3
					device pci c.0 off end # PCI E 2
					device pci d.0 off end # PCI E 1
					device pci e.0 on end # PCI E 0
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
					register "sata0_enable" = "1"
					register "sata1_enable" = "1"
					register "mac_eeprom_smbus" = "3" # 1: smbus under 2e.8, 2: SM0 3: SM1
					register "mac_eeprom_addr" = "0x51"
				end
			end #  device pci 18.0
			device pci 18.0 on end # Link 1
			device pci 18.0 on
			#  devices on link 2, link 2 == LDT 2
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on
						device pci 6.0 on end # lsi scsi
						device pci 6.1 on end
					end
					device pci 1.1 on end
				end
			end # device pci 18.0
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end #mc0

		chip northbridge/amd/amdk8
			device pci 19.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/nvidia/ck804
					device pci 0.0 on end   # HT
					device pci 1.0 on end   # LPC
					device pci 1.1 off end # SM
					device pci 2.0 off end # USB 1.1
					device pci 2.1 off end # USB 2
					device pci 4.0 off end # ACI
					device pci 4.1 off end # MCI
					device pci 6.0 off end # IDE
					device pci 7.0 off end # SATA 1
					device pci 8.0 off end # SATA 0
					device pci 9.0 off end # PCI
					device pci a.0 on end # NIC
					device pci b.0 off end # PCI E 3
					device pci c.0 off end # PCI E 2
					device pci d.0 off end # PCI E 1
					device pci e.0 on end # PCI E 0
					register "mac_eeprom_smbus" = "3"
					register "mac_eeprom_addr" = "0x51"
				end
			end #  device pci 19.0

			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.1 on end
			device pci 19.2 on end
			device pci 19.3 on end
		end
	end # PCI domain

#	chip drivers/generic/debug
#		device pnp 0.0 off end # chip name
#		device pnp 0.1 off end # pci_regs_all
#		device pnp 0.2 off end # mem
#		device pnp 0.3 off end # cpuid
#		device pnp 0.4 on  end # smbus_regs_all
#		device pnp 0.5 off end # dual core msr
#		device pnp 0.6 off end # cache size
#		device pnp 0.7 off end # tsc
#	end
end # root_complex
