chip northbridge/amd/amdfam10/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_F_1207
                        device apic 0 on end
                end
        end
	device pci_domain 0 on
		chip northbridge/amd/amdfam10 #mc0
			device pci 18.0 on end
			device pci 18.0 on end
			device pci 18.0 on 
        # SB on link 2.0
			        chip southbridge/nvidia/mcp55 
					device pci 0.0 on end   # HT
                			device pci 1.0 on # LPC
						chip superio/winbond/w83627hf
							device pnp 2e.0 off #  Floppy
                	                 			io 0x60 = 0x3f0
                	                			irq 0x70 = 6
                	                			drq 0x74 = 2
							end
                	        			device pnp 2e.1 off #  Parallel Port
                	                 			io 0x60 = 0x378
                	                			irq 0x70 = 7
							end
                	        			device pnp 2e.2 on #  Com1
                	                 			io 0x60 = 0x3f8
                	                			irq 0x70 = 4
							end
                	        			device pnp 2e.3 on #  Com2
                	                 			io 0x60 = 0x2f8
                	                			irq 0x70 = 3
							end
                	        			device pnp 2e.5 on #  Keyboard
                	                 			io 0x60 = 0x60
                	                 			io 0x62 = 0x64
                	                			irq 0x70 = 1
								irq 0x72 = 12
							end
                	        			device pnp 2e.6 off  # SFI 
                	                 			io 0x62 = 0x100
							end
                	        			device pnp 2e.7 off #  GPIO_GAME_MIDI
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end						
                	        			device pnp 2e.8 off end #  WDTO_PLED
                	        			device pnp 2e.9 off end #  GPIO_SUSLED
                	        			device pnp 2e.a off end #  ACPI
                	        			device pnp 2e.b on #  HW Monitor
 					 			io 0x60 = 0x290
								irq 0x70 = 5
                					end
						end
					end
			                device pci 1.1 on # SM 0
                                                chip drivers/generic/generic #dimm 0-0-0
                                                        device i2c 50 on end  
                                                end              
                                                chip drivers/generic/generic #dimm 0-0-1
                                                        device i2c 51 on end
                                                end     
                                                chip drivers/generic/generic #dimm 0-1-0
                                                        device i2c 52 on end
                                                end             
                                                chip drivers/generic/generic #dimm 0-1-1
                                                        device i2c 53 on end
                                                end              
                                                chip drivers/generic/generic #dimm 1-0-0
                                                        device i2c 54 on end
                                                end     
                                                chip drivers/generic/generic #dimm 1-0-1
                                                        device i2c 55 on end
                                                end     
                                                chip drivers/generic/generic #dimm 1-1-0
                                                        device i2c 56 on end
                                                end     
                                                chip drivers/generic/generic #dimm 1-1-1
                                                        device i2c 57 on end
                                                end 
					end # SM
                                        device pci 1.1 on # SM 1
#PCI device smbus address will depend on addon pci device, do we need to scan_smbus_bus?
#                                                chip drivers/generic/generic #PCIXA Slot1
#                                                        device i2c 50 on end
#                                                end
#                                                chip drivers/generic/generic #PCIXB Slot1
#                                                        device i2c 51 on end
#                                                end     
#                                                chip drivers/generic/generic #PCIXB Slot2
#                                                        device i2c 52 on end
#                                                end             
#                                                chip drivers/generic/generic #PCI Slot1
#                                                        device i2c 53 on end
#                                                end              
#                                                chip drivers/generic/generic #Master MCP55 PCI-E
#                                                        device i2c 54 on end
#                                                end     
#                                                chip drivers/generic/generic #Slave MCP55 PCI-E
#                                                        device i2c 55 on end
#                                                end             
                                                chip drivers/generic/generic #MAC EEPROM
                                                        device i2c 51 on end
                                                end 

                                        end # SM 
	                		device pci 2.0 on end # USB 1.1
        	        		device pci 2.1 on end # USB 2
                			device pci 4.0 on end # IDE
	                		device pci 5.0 on end # SATA 0
	                		device pci 5.1 on end # SATA 1
	                		device pci 5.2 on end # SATA 2
                			device pci 6.0 on  # PCI
                                                device pci 6.0 on end
					end
        	        		device pci 6.1 on end # AZA
	                		device pci 8.0 on end # NIC
	                		device pci 9.0 on end # NIC
        	       			device pci a.0 on  # PCI E 5
						device pci 0.0 on #nec pci-x
						end
						device pci 0.1 on #nec pci-x
							device pci 4.0 on end #scsi
							device pci 4.1 on end #scsi
						end
					end
        	       			device pci b.0 on end # PCI E 4
                			device pci c.0 on end # PCI E 3
                			device pci d.0 on end # PCI E 2
                			device pci e.0 on end # PCI E 1
        	       			device pci f.0 on end # PCI E 0
	                                register "ide0_enable" = "1"
                	                register "sata0_enable" = "1"
                        	        register "sata1_enable" = "1"
					register "mac_eeprom_smbus" = "3" # 1: smbus under 2e.8, 2: SM0 3: SM1
					register "mac_eeprom_addr" = "0x51"
				end
			end #  device pci 18.0 
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
			device pci 18.4 on end
			device pci 19.0 on end
			device pci 19.1 on end
			device pci 19.2 on end
			device pci 19.3 on end
			device pci 19.4 on end
		end # mc0
		
	end # PCI domain
	
#       chip drivers/generic/debug 
#               device pnp 0.0 off end # chip name
#                device pnp 0.1 on end # pci_regs_all
#                device pnp 0.2 off end # mem
#                device pnp 0.3 off end # cpuid
#                device pnp 0.4 on end # smbus_regs_all
#                device pnp 0.5 off end # dual core msr
#                device pnp 0.6 off end # cache size
#                device pnp 0.7 off end # tsc
#                device pnp 0.8 off  end # io
#                device pnp 0.9 on end # io
#       end  
end #root_complex
