/*
 * This file is part of the coreboot project.
 *
 * Minimalist ACPI DSDT table for EPIA-M / MII
 * (C) Copyright 2004 Nick Barker <Nick.Barker9@btinternet.com>
 *
 * (C) Copyright 2007 Rudolf Marek <r.marek@assembler.cz>
 *
 * ISA portions taken from QEMU acpi-dsdt.dsl  
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License v2 as published by
 * the Free Software Foundation.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 *
 * You should have received a copy of the GNU General Public License
 * along with this program; if not, write to the Free Software
 * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
 */


DefinitionBlock ("DSDT.aml", "DSDT", 1, "LXBIOS", "LXB-DSDT", 1)
{




	/*  
	 * Define the main processor
	 */
	Scope (\_PR)
	{
		Processor (\_PR.CPU0, 0x00, 0x000000, 0x00) {}
		Processor (\_PR.CPU1, 0x01, 0x000000, 0x00) {}
	}

	/* For now only define 2 power states:
	 *  - S0 which is fully on
	 *  - S5 which is soft off
	 * any others would involve declaring the wake up methods
	 */
	Name (\_S0, Package () {0x00, 0x00, 0x00, 0x00 })
	Name (\_S5, Package () {0x02, 0x02, 0x00, 0x00 })

	/* Root of the bus hierarchy */
	Scope (\_SB)
    	{
		/* top PCI device */
		Device (PCI0)
		{
			Name (_HID, EisaId ("PNP0A03"))
			Name (_ADR, 0x00)
			Name (_UID, 0x00)
			Name (_BBN, 0x00)
			
			/* PCI Routing Table */
			//aaa
			Name (_PRT, Package () {
	                    Package (0x04) { 0x000BFFFF, 0x00, 0x00, 0x10 }, //slot 0xB
        	            Package (0x04) { 0x000BFFFF, 0x01, 0x00, 0x11 },
                	    Package (0x04) { 0x000BFFFF, 0x02, 0x00, 0x12 },
	                    Package (0x04) { 0x000BFFFF, 0x03, 0x00, 0x13 },
        	            Package (0x04) { 0x000CFFFF, 0x00, 0x00, 0x11 }, //Slot 0xC
                	    Package (0x04) { 0x000CFFFF, 0x01, 0x00, 0x12 },
                	    Package (0x04) { 0x000CFFFF, 0x02, 0x00, 0x13 },
			    Package (0x04) { 0x000CFFFF, 0x03, 0x00, 0x10 },
        	            Package (0x04) { 0x000DFFFF, 0x00, 0x00, 0x12 }, //Slot 0xD
                	    Package (0x04) { 0x000DFFFF, 0x01, 0x00, 0x13 },
                	    Package (0x04) { 0x000DFFFF, 0x02, 0x00, 0x10 },
			    Package (0x04) { 0x000DFFFF, 0x03, 0x00, 0x11 },
        	            Package (0x04) { 0x000F0000, 0x01, 0x00, 0x14 }, //0xf SATA IRQ 20
                	    Package (0x04) { 0x000F0001, 0x00, 0x00, 0x14 }, //0xf NAtive IDE IRQ 20
        	            Package (0x04) { 0x0010FFFF, 0x00, 0x00, 0x15 }, //USB routing
                	    Package (0x04) { 0x0010FFFF, 0x01, 0x00, 0x15 },
                	    Package (0x04) { 0x0010FFFF, 0x02, 0x00, 0x15 },
			    Package (0x04) { 0x0010FFFF, 0x03, 0x00, 0x15 },
			    Package (0x04) { 0x0011FFFF, 0x02, 0x00, 0x16 }, //AC97 MC97
        	            Package (0x04) { 0x0002FFFF, 0x00, 0x00, 0x1B }, //PCIE16 bridge IRQ27
                	    Package (0x04) { 0x0002FFFF, 0x01, 0x00, 0x1B },
                	    Package (0x04) { 0x0002FFFF, 0x02, 0x00, 0x1B },
			    Package (0x04) { 0x0002FFFF, 0x03, 0x00, 0x1B },
        	            Package (0x04) { 0x0003FFFF, 0x00, 0x00, 0x1F }, //PCIE bridge IRQ31
                	    Package (0x04) { 0x0003FFFF, 0x01, 0x00, 0x23 }, //IRQ36
                	    Package (0x04) { 0x0003FFFF, 0x02, 0x00, 0x27 }, //IRQ39
			    Package (0x04) { 0x0003FFFF, 0x03, 0x00, 0x2B } //IRQ43
            		})

		
		Device (PEGG)
		{
			Name (_ADR, 0x00020000)
			Name (_UID, 0x00)
			Name (_BBN, 0x02)
			
			Name (_PRT, Package () {
	                    Package (0x04) { 0x0000FFFF, 0x00, 0x00, 0x18 }, //PCIE IRQ24-IRQ27
        	            Package (0x04) { 0x0000FFFF, 0x01, 0x00, 0x19 },
                	    Package (0x04) { 0x0000FFFF, 0x02, 0x00, 0x1A },
	                    Package (0x04) { 0x0000FFFF, 0x03, 0x00, 0x1B },
			})	
		} //end of PCIEG

		Device (PEX0)
		{
			Name (_ADR, 0x00030000)
			Name (_UID, 0x00)
			Name (_BBN, 0x03)
			
			Name (_PRT, Package () {
	                    Package (0x04) { 0x0000FFFF, 0x00, 0x00, 0x1C }, //PCIE IRQ28-IRQ31
        	            Package (0x04) { 0x0000FFFF, 0x01, 0x00, 0x1D },
                	    Package (0x04) { 0x0000FFFF, 0x02, 0x00, 0x1E },
	                    Package (0x04) { 0x0000FFFF, 0x03, 0x00, 0x1F },
			})	
		} //end of PEX0

		Device (PEX1)
		{
			Name (_ADR, 0x00030001)
			Name (_UID, 0x00)
			Name (_BBN, 0x04)
			
			Name (_PRT, Package () {
	                    Package (0x04) { 0x0000FFFF, 0x00, 0x00, 0x20 }, //PCIE IRQ32-IRQ35
        	            Package (0x04) { 0x0000FFFF, 0x01, 0x00, 0x21 },
                	    Package (0x04) { 0x0000FFFF, 0x02, 0x00, 0x22 },
	                    Package (0x04) { 0x0000FFFF, 0x03, 0x00, 0x23 },
			})	
		} //end f PEX1

		Device (PEX2)
		{
			Name (_ADR, 0x00030002)
			Name (_UID, 0x00)
			Name (_BBN, 0x05)
			
			Name (_PRT, Package () {
	                    Package (0x04) { 0x0000FFFF, 0x00, 0x00, 0x24 }, //PCIE IRQ36-IRQ39
        	            Package (0x04) { 0x0000FFFF, 0x01, 0x00, 0x25 },
                	    Package (0x04) { 0x0000FFFF, 0x02, 0x00, 0x26 },
	                    Package (0x04) { 0x0000FFFF, 0x03, 0x00, 0x27 },
			})	
		} //end f PEX2

		Device (PEX3)
		{
			Name (_ADR, 0x00030003)
			Name (_UID, 0x00)
			Name (_BBN, 0x06)
			
			Name (_PRT, Package () {
	                    Package (0x04) { 0x0000FFFF, 0x00, 0x00, 0x28 }, //PCIE IRQ40-IRQ43
        	            Package (0x04) { 0x0000FFFF, 0x01, 0x00, 0x29 },
                	    Package (0x04) { 0x0000FFFF, 0x02, 0x00, 0x2A },
	                    Package (0x04) { 0x0000FFFF, 0x03, 0x00, 0x2B },
			})	
		} //end f PEX3

        Device (ISA) {
            Name (_ADR, 0x00110000)
        
            /* Keyboard seems to be important for WinXP install */
            Device (KBD)
            {
                Name (_HID, EisaId ("PNP0303"))
                Method (_STA, 0, NotSerialized)
                {
                    Return (0x0f)
                }

                Method (_CRS, 0, NotSerialized)
                {
                     Name (TMP, ResourceTemplate ()
                     {
                    IO (Decode16,
                        0x0060,             // Address Range Minimum
                        0x0060,             // Address Range Maximum
                        0x01,               // Address Alignment
                        0x01,               // Address Length
                        )
                    IO (Decode16,
                        0x0064,             // Address Range Minimum
                        0x0064,             // Address Range Maximum
                        0x01,               // Address Alignment
                        0x01,               // Address Length
                        )
                    IRQNoFlags ()
                        {1}
                    })
                    Return (TMP)
                }
            }

	    /* PS/2 mouse */
            Device (MOU) 
            {
                Name (_HID, EisaId ("PNP0F13"))
                Method (_STA, 0, NotSerialized)
                {
                    Return (0x0f)
                }

                Method (_CRS, 0, NotSerialized)
                {
                    Name (TMP, ResourceTemplate ()
                    {
                         IRQNoFlags () {12}
                    })
                    Return (TMP)
                }
            }

	    /* PS/2 floppy controller */
	    Device (FDC0)
	    {
	        Name (_HID, EisaId ("PNP0700"))
		Method (_STA, 0, NotSerialized)
		{
		    Return (0x0F)
		}
		Method (_CRS, 0, NotSerialized)
		{
		    Name (BUF0, ResourceTemplate ()
                    {
                        IO (Decode16, 0x03F2, 0x03F2, 0x00, 0x04)
                        IO (Decode16, 0x03F7, 0x03F7, 0x00, 0x01)
                        IRQNoFlags () {6}
                        DMA (Compatibility, NotBusMaster, Transfer8) {2}
                    })
		    Return (BUF0)
		}
	    } //FD END

        } //ISA END

	} // End of PCI0
		
		
	} // End of _SB

} // End of Definition Block

