##
## This file is part of the coreboot project.
##
## Copyright (C) 2007 Uwe Hermann <uwe@hermann-uwe.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

if USE_FALLBACK_IMAGE
	default ROM_SECTION_SIZE = FALLBACK_SIZE
	default ROM_SECTION_OFFSET = (ROM_SIZE - FALLBACK_SIZE)
else
	default ROM_SECTION_SIZE = (ROM_SIZE - FALLBACK_SIZE)
	default ROM_SECTION_OFFSET = 0
end
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE
				    + ROM_SECTION_OFFSET + 1)
default PAYLOAD_SIZE = (ROM_SECTION_SIZE - ROM_IMAGE_SIZE)
default _ROMBASE = (CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE)
default XIP_ROM_SIZE = 64 * 1024
default XIP_ROM_BASE = (_ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE)
arch i386 end
driver mainboard.o
if HAVE_PIRQ_TABLE
	object irq_tables.o
end
makerule ./failover.E
	depends "$(MAINBOARD)/../../../arch/i386/lib/failover.c ./romcc"
	action "./romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/../../../arch/i386/lib/failover.c -o $@"
end
makerule ./failover.inc
	depends "$(MAINBOARD)/../../../arch/i386/lib/failover.c ./romcc"
	action "./romcc -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/../../../arch/i386/lib/failover.c -o $@"
end
makerule ./auto.E
	# depends	"$(MAINBOARD)/auto.c option_table.h ./romcc"
	depends	"$(MAINBOARD)/auto.c ./romcc"
	action	"./romcc -E -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc
	# depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
	depends "$(MAINBOARD)/auto.c ./romcc"
	action	"./romcc -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
ldscript /cpu/x86/32bit/entry32.lds
if USE_FALLBACK_IMAGE
	mainboardinit cpu/x86/16bit/reset16.inc
	ldscript /cpu/x86/16bit/reset16.lds
else
	mainboardinit cpu/x86/32bit/reset32.inc
	ldscript /cpu/x86/32bit/reset32.lds
end
mainboardinit arch/i386/lib/cpu_reset.inc
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds
if USE_FALLBACK_IMAGE
	ldscript /arch/i386/lib/failover.lds
	mainboardinit ./failover.inc
end
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc

dir /pc80
config chip.h

chip northbridge/intel/i440bx		# Northbridge
  device apic_cluster 0 on		# APIC cluster
    chip cpu/intel/slot_2		# CPU (FIXME: It's slot 1, actually)
      device apic 0 on end		# APIC
    end
  end
  device pci_domain 0 on		# PCI domain
    device pci 0.0 on end		# Host bridge
    device pci 1.0 on end		# PCI/AGP bridge
    chip southbridge/intel/i82371eb	# Southbridge
      device pci 7.0 on			# ISA bridge
        chip superio/winbond/w83977tf	# Super I/O (FIXME: It's W83977EF!)
          device pnp 3f0.0 on		# Floppy
            io 0x60 = 0x3f0
            irq 0x70 = 6
            drq 0x74 = 2
          end
          device pnp 3f0.1 on		# Parallel port
            io 0x60 = 0x378
            irq 0x70 = 7
          end
          device pnp 3f0.2 on		# COM1
            io 0x60 = 0x3f8
            irq 0x70 = 4
          end
          device pnp 3f0.3 on		# COM2 / IR
            io 0x60 = 0x2f8
            irq 0x70 = 3
          end
          device pnp 3f0.5 on		# PS/2 keyboard / mouse
            io 0x60 = 0x60
            io 0x62 = 0x64
            irq 0x70 = 1		# PS/2 keyboard interrupt
            irq 0x72 = 12		# PS/2 mouse interrupt
          end
          device pnp 3f0.6 on		# Consumer IR
          end
          device pnp 3f0.7 on		# GPIO 1
          end
          device pnp 3f0.8 on		# GPIO 2
          end
          device pnp 3f0.a on		# ACPI
          end
        end
      end
      device pci 7.1 on	end		# IDE
      device pci 7.2 on	end		# USB
      device pci 7.3 on end		# ACPI
      register "ide0_enable" = "1"
      register "ide1_enable" = "1"
      register "ide_legacy_enable" = "1"
      # Enable UDMA/33 for higher speed if your IDE device(s) support it.
      register "ide0_drive0_udma33_enable" = "0"
      register "ide0_drive1_udma33_enable" = "0"
      register "ide1_drive0_udma33_enable" = "0"
      register "ide1_drive1_udma33_enable" = "0"
    end
  end
end
