##
## Compute the location and size of where this firmware image
## (coreboot plus bootloader) will live in the boot rom chip.
##
if USE_FALLBACK_IMAGE
	default ROM_SECTION_SIZE   = FALLBACK_SIZE
	default ROM_SECTION_OFFSET = ( ROM_SIZE - FALLBACK_SIZE )
else
	default ROM_SECTION_SIZE   = ( ROM_SIZE - FALLBACK_SIZE )
	default ROM_SECTION_OFFSET = 0
end

##
## Compute the start location and size size of
## The coreboot bootloader.
##
default PAYLOAD_SIZE            = ( ROM_SECTION_SIZE - ROM_IMAGE_SIZE )
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)

##
## Compute where this copy of coreboot will start in the boot rom
##
default _ROMBASE      = ( CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE )

##
## Compute a range of ROM that can cached to speed up coreboot,
## execution speed.
##
## XIP_ROM_SIZE must be a power of 2.
## XIP_ROM_BASE must be a multiple of XIP_ROM_SIZE
##
default XIP_ROM_SIZE=65536
default XIP_ROM_BASE = ( _ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE )

arch i386 end 

##
## Build the objects we have code for in this directory.
##

driver mainboard.o

#dir /drivers/si/3114

if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE 
	object get_bus_conf.o
	object irq_tables.o 
end

#object reset.o

if USE_DCACHE_RAM

	if CONFIG_USE_INIT

		makerule ./cache_as_ram_auto.o
			depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
			action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -o $@" 
		end

	else    
                
		makerule ./cache_as_ram_auto.inc
			depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
			action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -S -o $@"         
			action "perl -e 's/.rodata/.rom.data/g' -pi $@"
			action "perl -e 's/.text/.section .rom.text/g' -pi $@"
		end

	end

end
##
## Build our 16 bit and 32 bit coreboot entry code
##
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
if USE_DCACHE_RAM
        if CONFIG_USE_INIT
                ldscript /cpu/x86/32bit/entry32.lds
        end

        if CONFIG_USE_INIT
                ldscript      /cpu/amd/car/cache_as_ram.lds
        end
end

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

if USE_DCACHE_RAM
	##
	## Setup Cache-As-Ram
	##
	mainboardinit cpu/amd/car/cache_as_ram.inc
end

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
	if USE_DCACHE_RAM
	       ldscript /arch/i386/lib/failover.lds
	else
	       ldscript /arch/i386/lib/failover.lds
		mainboardinit ./failover.inc
	end
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
if USE_DCACHE_RAM

	if CONFIG_USE_INIT
		initobject cache_as_ram_auto.o
	else
		mainboardinit ./cache_as_ram_auto.inc
	end

end

##
## Include the secondary Configuration files 
##
if CONFIG_CHIP_NAME
	config chip.h
end

# sample config for broadcom/blast 
chip northbridge/amd/amdk8/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_940
                        device apic 0 on end
                end
        end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge 
                              #  devices on link 0
                                chip southbridge/broadcom/bcm5780 # HT2000
                                        device pci 0.0 on end   # PXB 1 0x0130
                                        device pci 1.0 on       # PXB 2 0x0130
                                                device pci 4.0 on end # GB E 0x1668 vid = 0x14e4
                                                device pci 4.1 on end # GB E 0x1669 vid = 0x14e4
                                        end
                                        device pci 2.0 on end # PCI E 1  #0x0132
                                        device pci 3.0 on end # PCI E 2
                                        device pci 4.0 on end # PCI E 3
                                        device pci 5.0 on end # PCI E 4
                                end
                                chip southbridge/broadcom/bcm5785 # HT1000
                                        device pci 0.0 on  # HT PXB  0x0036
                                                device pci d.0 on end # PPBX 0x0104
                                                device pci e.0 on end # SATA 0x024a
                                        end
                                        device pci 1.0 on # Legacy  pci main  0x0205
                                                chip drivers/i2c/i2cmux2 # pca9554 smbus mux
                                                        device i2c 71 on end #0 pca9554 0
							device i2c 71 on end #0 pca9554 1
							device i2c 71 on end #0 pca9554 2
							device i2c 71 on end #0 pca9554 3
							device i2c 71 on end #0 pca9554 4
							device i2c 71 on end #0 pca9554 5
                                                        device i2c 71 on #0 pca9554 6
                                                                chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 50 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 51 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 52 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 53 on end
                                                                end
                                                        end
                                                        device i2c 71 on #1 pca9554 7
                                                                chip drivers/generic/generic #dimm 1-0-0
                                                                        device i2c 50 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 1-0-1
                                                                        device i2c 51 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 1-1-0
                                                                        device i2c 52 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 1-1-1
                                                                        device i2c 53 on end
                                                                end
                                                        end
                                                end

					end
                                        device pci 1.1 on end # IDE        0x0214
                                        device pci 1.2 on     # LPC        0x0234
                                                chip superio/nsc/pc87417
                                                        device  pnp 2e.0 off  # Floppy
                                                                 io 0x60 = 0x3f0
                                                                irq 0x70 = 6
                                                                drq 0x74 = 2
                                                        end
                                                        device pnp 2e.1 off  # Parallel Port
                                                                 io 0x60 = 0x378
                                                                irq 0x70 = 7
                                                        end
                                                        device pnp 2e.2 off # Com 2
                                                                 io 0x60 = 0x2f8
                                                                irq 0x70 = 3
                                                        end
                                                        device pnp 2e.3 on  # Com 1
                                                                 io 0x60 = 0x3f8
                                                                irq 0x70 = 4
                                                        end
                                                        device pnp 2e.4 off end # SWC
                                                        device pnp 2e.5 off end # Mouse
                                                        device pnp 2e.6 on  # Keyboard
                                                                 io 0x60 = 0x60
                                                                 io 0x62 = 0x64
                                                                irq 0x70 = 1
                                                        end
                                                        device pnp 2e.7 off end # GPIO
                                                        device pnp 2e.f off end # XBUS
                                                        device pnp 2e.10 on #RTC
								 io 0x60 = 0x70
								 io 0x62 = 0x72
							end 
                                                end
                                        end
                                        device pci 1.3 on end # WDTimer    0x0238
                                        device pci 1.4 on end # XIOAPIC0   0x0235
                                        device pci 1.5 on end # XIOAPIC1
                                        device pci 1.6 on end # XIOAPIC2
                                        device pci 2.0 on end # USB        0x0223
                                        device pci 2.1 on end # USB
                                        device pci 2.2 on end # USB
                                        #when HT_CHAIN_END_UNITID_BASE (0,1) < HT_CHAIN_UNITID_BASE (6,,,,),
                                        chip drivers/pci/onboard
                                              device pci 4.0 on end # it is in bcm5785_0 bus, but the device id can not be changed even unitid is changed, fake one to get the rom_address
                                                                    # if HT_CHAIN_END_UNITID_BASE=0, it is 5, if HT_CHAIN_END_UNITID_BASE=1, it is 4
                                              register "rom_address" = "0xfff80000"
                                        end
                                end
                                        #when HT_CHAIN_END_UNITID_BASE > HT_CHAIN_UNITID_BASE (6, ,,,,)
#                                        chip drivers/pci/onboard
#                                              device pci 0.0 on end # fake, will be disabled
#                                        end
#                                        chip drivers/pci/onboard
#                                              device pci 5.0 on end # it is in bcm5785_0 bus, but the device id can not be changed even unitid is changed
#                                              register "rom_address" = "0xfff80000"
#                                        end


			end #  device pci 18.0

                        device pci 18.0 on end
                        device pci 18.0 on end  
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end


	end #pci_domain
#        chip drivers/generic/debug
#                device pnp 0.0 off end # chip name
#                device pnp 0.1 on end # pci_regs_all
#                device pnp 0.2 off end # mem
#                device pnp 0.3 off end # cpuid
#                device pnp 0.4 off end # smbus_regs_all
#                device pnp 0.5 off end # dual core msr
#                device pnp 0.6 off end # cache size
#                device pnp 0.7 off end # tsc
#       end

end

