##
## This file is part of the coreboot project.
##
## Copyright (C) 2007 Uwe Hermann <uwe@hermann-uwe.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

if USE_FAILOVER_IMAGE
  default ROM_SECTION_SIZE   = FAILOVER_SIZE
  default ROM_SECTION_OFFSET = (ROM_SIZE - FAILOVER_SIZE)
else
  if USE_FALLBACK_IMAGE
    default ROM_SECTION_SIZE   = FALLBACK_SIZE
    default ROM_SECTION_OFFSET = (ROM_SIZE - FALLBACK_SIZE - FAILOVER_SIZE)
  else
    default ROM_SECTION_SIZE   = (ROM_SIZE - FALLBACK_SIZE - FAILOVER_SIZE)
    default ROM_SECTION_OFFSET = 0
  end
end

default PAYLOAD_SIZE = (ROM_SECTION_SIZE - ROM_IMAGE_SIZE)
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)
default _ROMBASE = (CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE)
default XIP_ROM_SIZE = 65536

if USE_FAILOVER_IMAGE
  default XIP_ROM_BASE = (_ROMBASE - XIP_ROM_SIZE + ROM_IMAGE_SIZE)
else
  if USE_FALLBACK_IMAGE
    default XIP_ROM_BASE = (_ROMBASE - XIP_ROM_SIZE + ROM_IMAGE_SIZE + FAILOVER_SIZE)
  else
    default XIP_ROM_BASE = (_ROMBASE - XIP_ROM_SIZE + ROM_IMAGE_SIZE)
  end
end

arch i386 end

driver mainboard.o
object get_bus_conf.o # Needed by irq_tables and mptable (and acpi_tables).
if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
# object reset.o

if USE_DCACHE_RAM
  if CONFIG_USE_INIT
    makerule ./cache_as_ram_auto.o
      depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
      action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -o $@"
    end
  else
    makerule ./cache_as_ram_auto.inc
      depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
      action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -S -o $@"
      action "perl -e 's/.rodata/.rom.data/g' -pi $@"
      action "perl -e 's/.text/.section .rom.text/g' -pi $@"
    end
  end
end

if USE_FAILOVER_IMAGE
else
  if CONFIG_AP_CODE_IN_CAR
    makerule ./apc_auto.o
      depends "$(MAINBOARD)/apc_auto.c option_table.h"
      action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/apc_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -o $@"
    end
    ldscript /arch/i386/init/ldscript_apc.lb
  end
end

if HAVE_FAILOVER_BOOT
  if USE_FAILOVER_IMAGE
    mainboardinit cpu/x86/16bit/entry16.inc
    ldscript /cpu/x86/16bit/entry16.lds
  end
else
  if USE_FALLBACK_IMAGE
    mainboardinit cpu/x86/16bit/entry16.inc
    ldscript /cpu/x86/16bit/entry16.lds
  end
end

mainboardinit cpu/x86/32bit/entry32.inc

if USE_DCACHE_RAM
  if CONFIG_USE_INIT
    ldscript /cpu/x86/32bit/entry32.lds
  end
  if CONFIG_USE_INIT
    ldscript /cpu/amd/car/cache_as_ram.lds
  end
end

if HAVE_FAILOVER_BOOT
  if USE_FAILOVER_IMAGE
    mainboardinit cpu/x86/16bit/reset16.inc
    ldscript /cpu/x86/16bit/reset16.lds
  else
    mainboardinit cpu/x86/32bit/reset32.inc
    ldscript /cpu/x86/32bit/reset32.lds
  end
else
  if USE_FALLBACK_IMAGE
    mainboardinit cpu/x86/16bit/reset16.inc
    ldscript /cpu/x86/16bit/reset16.lds
  else
    mainboardinit cpu/x86/32bit/reset32.inc
    ldscript /cpu/x86/32bit/reset32.lds
  end
end

mainboardinit southbridge/nvidia/mcp55/id.inc
ldscript /southbridge/nvidia/mcp55/id.lds

# ROMSTRAP table for MCP55.
if HAVE_FAILOVER_BOOT
  if USE_FAILOVER_IMAGE
    mainboardinit southbridge/nvidia/mcp55/romstrap.inc
    ldscript /southbridge/nvidia/mcp55/romstrap.lds
  end
else
  if USE_FALLBACK_IMAGE
    mainboardinit southbridge/nvidia/mcp55/romstrap.inc
    ldscript /southbridge/nvidia/mcp55/romstrap.lds
  end
end

if USE_DCACHE_RAM
  mainboardinit cpu/amd/car/cache_as_ram.inc
end

if HAVE_FAILOVER_BOOT
  if USE_FAILOVER_IMAGE
    if USE_DCACHE_RAM
      ldscript /arch/i386/lib/failover_failover.lds
    end
  end
else
  if USE_FALLBACK_IMAGE
    if USE_DCACHE_RAM
      ldscript /arch/i386/lib/failover.lds
    end
  end
end

if USE_DCACHE_RAM
  if CONFIG_USE_INIT
    initobject cache_as_ram_auto.o
  else
    mainboardinit ./cache_as_ram_auto.inc
  end
end

if CONFIG_CHIP_NAME
  config chip.h
end

chip northbridge/amd/amdk8/root_complex		# Root complex
  device apic_cluster 0 on			# APIC cluster
    chip cpu/amd/socket_AM2			# CPU
      device apic 0 on end			# APIC
    end
  end
  device pci_domain 0 on			# PCI domain
    chip northbridge/amd/amdk8			# Northbridge / mc0
      device pci 18.0 on
        # Devices on link 0, link 0 == LDT 0
        chip southbridge/nvidia/mcp55		# Southbridge
          device pci 0.0 on end			# HT
          device pci 1.0 on			# LPC
            chip superio/winbond/w83627ehg	# Super I/O
              device pnp 4e.0 on		# Floppy
                io 0x60 = 0x3f0
                irq 0x70 = 6
                drq 0x74 = 2
              end
              device pnp 4e.1 on		# Parallel port
                io 0x60 = 0x378
                irq 0x70 = 7
              end
              device pnp 4e.2 on		# Com1
                io 0x60 = 0x3f8
                irq 0x70 = 4
              end
              device pnp 4e.3 on		# Com2 / IrDA
                io 0x60 = 0x2f8
                irq 0x70 = 3
              end
              device pnp 4e.5 on		# PS/2 keyboard
                io 0x60 = 0x60
                io 0x62 = 0x64
                irq 0x70 = 1			# PS/2 keyboard IRQ
                irq 0x72 = 12			# PS/2 mouse IRQ
              end
              device pnp 4e.6 off		# Serial flash interface
                # io 0x62 = 0x100
              end
              device pnp 4e.7 off		# GPIO1/6, game port, MIDI port
                # io 0x60 = 0x220		# Datasheet: 0x201
                # io 0x62 = 0x300		# Datasheet: 0x330
                # irq 0x70 = 9
              end
              device pnp 4e.8 off		# WDTO#, PLED
              end
              device pnp 4e.9 off		# GPIO2/3/4/5, SUSLED
              end
              device pnp 4e.a off		# ACPI
              end
              device pnp 4e.b on		# HWM (for lm-sensors)
                io 0x60 = 0xa10
              end
            end
          end
          device pci 1.1 on			# SM 0
            chip drivers/generic/generic	# DIMM 0-0-0
              device i2c 50 on end
            end
            chip drivers/generic/generic	# DIMM 0-0-1
              device i2c 51 on end
            end
            chip drivers/generic/generic	# DIMM 0-1-0
              device i2c 52 on end
            end
            chip drivers/generic/generic	# DIMM 0-1-1
              device i2c 53 on end
            end
            # TODO: Needed?
            # chip drivers/generic/generic	# DIMM 1-0-0
            #   device i2c 54 on end
            # end
            # chip drivers/generic/generic	# DIMM 1-0-1
            #   device i2c 55 on end
            # end
            # chip drivers/generic/generic	# DIMM 1-1-0
            #   device i2c 56 on end
            # end
            # chip drivers/generic/generic	# DIMM 1-1-1
            #   device i2c 57 on end
            # end
          end
          # TODO: Check if the stuff below is correct / needed.
          device pci 1.1 on			# SM 1
            # PCI device SMBus address will depend on addon PCI device,
            # do we need to scan_smbus_bus?

            # chip drivers/generic/generic	# PCIXA Slot1
            #   device i2c 50 on end
            # end
            # chip drivers/generic/generic	# PCIXB Slot1
            #   device i2c 51 on end
            # end
            # chip drivers/generic/generic	# PCIXB Slot2
            #   device i2c 52 on end
            # end
            # chip drivers/generic/generic	# PCI Slot1
            #   device i2c 53 on end
            # end
            # chip drivers/generic/generic	# Master MCP55 PCI-E
            #   device i2c 54 on end
            # end
            # chip drivers/generic/generic	# Slave MCP55 PCI-E
            #   device i2c 55 on end
            # end
            chip drivers/generic/generic	# MAC EEPROM
              device i2c 51 on end
            end
          end
          device pci 2.0 on end			# USB 1.1
          device pci 2.1 on end			# USB 2
          device pci 4.0 on end			# IDE
          device pci 5.0 on end			# SATA 0
          device pci 5.1 on end			# SATA 1
          device pci 5.2 off end		# SATA 2 (N/A on this board)
          device pci 6.0 on end			# PCI
          device pci 6.1 on end			# AZA (HD Audio)
          device pci 8.0 on end			# NIC
          device pci 9.0 off end		# NIC (N/A on this board)
          device pci a.0 off end		# PCI E 5 (N/A on this board?)
          device pci b.0 on end			# PCI E 4
          device pci c.0 on end			# PCI E 3
          device pci d.0 on end			# PCI E 2
          device pci e.0 on end			# PCI E 1
          device pci f.0 on end			# PCI E 0
          register "ide0_enable" = "1"
          register "sata0_enable" = "1"
          register "sata1_enable" = "1"
          # TODO: Check the two lines below.
          register "mac_eeprom_smbus" = "3"	# 1: SMBus under 2e.8, 2: SM0 3: SM1
          register "mac_eeprom_addr" = "0x51"
        end
      end
      device pci 18.0 on end			# Link 1
      device pci 18.0 on end
      device pci 18.1 on end
      device pci 18.2 on end
      device pci 18.3 on end
    end
  end

# TODO
#  chip drivers/generic/debug
#    device pnp 0.0 off end			# chip name
#    device pnp 0.1 on end			# pci_regs_all
#    device pnp 0.2 on end			# mem
#    device pnp 0.3 off end			# cpuid
#    device pnp 0.4 on end			# smbus_regs_all
#    device pnp 0.5 off end			# dual core msr
#    device pnp 0.6 off end			# cache size
#    device pnp 0.7 off end			# tsc
#    device pnp 0.8 off end			# io
#    device pnp 0.9 off end			# io
#  end

end
