#######################################################
#
# Main options file for coreboot
#
# Each option used by a part must be defined in
# this file. The format for options is:
#
#   define <name> 
#	default <expr> | {<expr>} | "<string>" | none
#	format "<string>"
#	export always | used | never
#	comment "<string>"
#   end
#
# where 
#
#   <name> is the name of the option
#   <expr> is a numeric expression
#   <string> is a string
#
# Either a default value or 'default none' must
# be specified for every option. An option
# specified as 'default none' will not be exported
# (i.e. will remain undefined) unless it has
# been assigned a value.
#
# Option values can be an immediate expression that 
# evaluates to a numeric value, a delayed expression 
# (surrounded by curley braces), or a string 
# (surrounded by double quotes.)
#
# Immediate expressions are evaluated at the time an
# option is defined or set and the numeric result 
# becomes the value of the option.
#
# Delayed expression are evaluated at the time the 
# option is used, either in another expression or 
# when being exported.
#
# String values will have the double quotes removed 
# automatically. 
#
# Format strings determine the print format that is 
# used when exporting options. The default format
# is "%s" for strings and "%d" for numbers.
#
# Exported options generate entries in the 
# Makefile.settings file. Options can be always 
# exported, exported only if used, or never exported.
#
# A comment string must be supplied for every option.
#
#######################################################

###############################################
# Architecture options
###############################################

define ARCH
	default "i386"
	export always
	comment "Default architecture is i386, options are alpha and ppc"
end
define HAVE_MOVNTI
	default 0
	export always
	comment "This cpu supports the MOVNTI directive"
end

###############################################
# Build options
###############################################

define CROSS_COMPILE
	default ""
	export always
	comment "Cross compiler prefix"
end
define CC
	default "$(CROSS_COMPILE)gcc"
	export always
	comment "Target C Compiler"
end
define HOSTCC
	default "gcc"
	export always
	comment "Host C Compiler"
end
define CPU_OPT
	default none
	export used
	comment "Additional per-cpu CFLAGS"
end
define OBJCOPY
	default "$(CROSS_COMPILE)objcopy --gap-fill 0xff"
	export always
	comment "Objcopy command"
end
define COREBOOT_VERSION
	default "2.0.0"
	export always
	format "\"%s\""
	comment "coreboot version"
end
define COREBOOT_EXTRA_VERSION
        default ""
        export used
	format "\"%s\""
        comment "coreboot extra version"
end
define COREBOOT_BUILD
	default "$(shell date)"
	export always
	format "\"%s\""
	comment "Build date"
end
define COREBOOT_COMPILE_TIME
	default "$(shell date +%T)"
	export always
	format "\"%s\""
	comment "Build time"
end
define COREBOOT_COMPILE_BY
	default "$(shell whoami)"
	export always
	format "\"%s\""
	comment "Who build this image"
end
define COREBOOT_COMPILE_HOST
	default "$(shell hostname)"
	export always
	format "\"%s\""
	comment "Build host"
end

define COREBOOT_COMPILE_DOMAIN
	default "$(shell dnsdomainname)"
	export always
	format "\"%s\""
	comment "Build domain name"
end
define COREBOOT_COMPILER
	default "$(shell $(CC) $(CFLAGS) -v 2>&1 | tail -n 1)"
	export always
	format "\"%s\""
	comment "Build compiler"
end
define COREBOOT_LINKER
	default "$(shell  $(CC) -Wl,--version 2>&1 | grep version | tail -n 1)"
	export always
	format "\"%s\""
	comment "Build linker"
end
define COREBOOT_ASSEMBLER
	default "$(shell  touch dummy.s ; $(CC) -c -Wa,-v dummy.s 2>&1; rm -f dummy.s dummy.o )"
	export always
	format "\"%s\""
	comment "Build assembler"
end
define CONFIG_CHIP_CONFIGURE
	default 0
	export used
	comment "Use new chip_configure method for configuring (non-pci) devices"
end
define CONFIG_USE_INIT
	default 0
	export always
	comment "Use stage 1 initialization code"
end

###############################################
# ROM image options
###############################################

define HAVE_FALLBACK_BOOT
	format "%d"
	default 0
	export always
	comment "Set if fallback booting required"
end
define HAVE_FAILOVER_BOOT
	format "%d"
	default 0
	export always
	comment "Set if failover booting required"
end
define USE_FALLBACK_IMAGE
	format "%d"
	default 0
	export used
	comment "Set to build a fallback image"
end
define USE_FAILOVER_IMAGE
        format "%d"
        default 0
        export used
        comment "Set to build a failover image"
end
define FALLBACK_SIZE
	default 65536
	format "0x%x"
	export used
	comment "Default fallback image size"
end
define FAILOVER_SIZE
        default 0
        format "0x%x"
        export used
        comment "Default failover image size"
end
define ROM_SIZE
	default none
	format "0x%x"
	export used
	comment "Size of your ROM"
end
define ROM_IMAGE_SIZE
	default 65535
	format "0x%x"
	export always
	comment "Default image size"
end
define ROM_SECTION_SIZE
	default {FALLBACK_SIZE}
	format "0x%x"
	export used
	comment "Default rom section size"
end
define ROM_SECTION_OFFSET
	default {ROM_SIZE - FALLBACK_SIZE}
	format "0x%x"
	export used
	comment "Default rom section offset"
end
define PAYLOAD_SIZE
	default {ROM_SECTION_SIZE - ROM_IMAGE_SIZE}
	format "0x%x"
	export always
	comment "Default payload size"
end
define _ROMBASE
	default {PAYLOAD_SIZE}
	format "0x%x"
	export always
	comment "Base address of coreboot in ROM"
end
define _ROMSTART
	default none
	format "0x%x"
	export used
	comment "Start address of coreboot in ROM"
end
define _RESET
	default {_ROMBASE}
	format "0x%x"
	export always
	comment "Hardware reset vector address"
end
define _EXCEPTION_VECTORS
	default {_ROMBASE+0x100}
	format "0x%x"
	export always
	comment "Address of exception vector table"
end
define STACK_SIZE
	default 0x2000
	format "0x%x"
	export always
	comment "Default stack size"
end
define HEAP_SIZE
	default 0x2000
	format "0x%x"
	export always
	comment "Default heap size"
end
define _RAMBASE
	default none
	format "0x%x"
	export always
	comment "Base address of coreboot in RAM"
end
define _RAMSTART
	default none
	format "0x%x"
	export used
	comment "Start address of coreboot in RAM"
end
define USE_DCACHE_RAM
	default 0
	export always
	comment "Use data cache as temporary RAM if possible"
end
define CAR_FAM10
	default 0
	export always
	comment "AMD family 10 CAR requires additional setup"
end
define DCACHE_RAM_BASE
	default 0xc0000
	format "0x%x"
	export always
	comment "Base address of data cache when using it for temporary RAM"
end
define DCACHE_RAM_SIZE
	default 0x1000
	format "0x%x"
	export always
	comment "Size of data cache when using it for temporary RAM"
end
define DCACHE_RAM_GLOBAL_VAR_SIZE
	default 0
	format "0x%x"
	export always
	comment "Size of region that for global variable of cache as ram stage"
end
define CONFIG_AP_CODE_IN_CAR
        default 0
        export always
        comment "will copy coreboot_apc to AP cache ane execute in AP"
end
define MEM_TRAIN_SEQ
        default 0
        export always
        comment "0: three for in bsp, 1: on every core0, 2: one for on bsp"
end
define WAIT_BEFORE_CPUS_INIT
        default 0
        export always
        comment "execute cpus_ready_for_init if it is set to 1"
end
define XIP_ROM_BASE
	default 0
	format "0x%x"
	export used
	comment "Start address of area to cache during coreboot execution directly from ROM"
end
define XIP_ROM_SIZE
	default 0
	format "0x%x"
	export used
	comment "Size of area to cache during coreboot execution directly from ROM"
end
define CONFIG_COMPRESS
	default 1
	export always
	comment "Set for compressed image"
end
define CONFIG_UNCOMPRESSED
	format "%d"
	default {!CONFIG_COMPRESS}
	export always
	comment "Set for uncompressed image"
end
define CONFIG_LB_MEM_TOPK
	format "%d"
	default 2048
	export always
	comment "Kilobytes of memory to initialized before executing code from RAM"
end
define HAVE_OPTION_TABLE
	default 0
	export always
	comment "Export CMOS option table"
end
define USE_OPTION_TABLE
	format "%d"
	default {HAVE_OPTION_TABLE && !USE_FALLBACK_IMAGE}
	export always
	comment "Use option table"
end

###############################################
# CMOS variable options
###############################################
define LB_CKS_RANGE_START
	default 49
	format "%d"
	export always
	comment "First CMOS byte to use for coreboot options"
end
define LB_CKS_RANGE_END
	default 125
	format "%d"
	export always
	comment "Last CMOS byte to use for coreboot options"
end
define LB_CKS_LOC
	default 126
	format "%d"
	export always
	comment "Pair of bytes to use for CMOS checksum"
end


###############################################
# Build targets
###############################################

define CRT0
	default "$(TOP)/src/arch/$(ARCH)/init/crt0.S.lb"
	export always
	comment "Main initialization target"
end

###############################################
# Debugging/Logging options
###############################################

define DEBUG
	default 1
	export always
	comment "Enable debugging code"
end
define CONFIG_CONSOLE_VGA
	default 0
	export always
	comment "Log messages to any VGA-compatible device (may require *_ROM_RUN to bring up)"
end
define CONFIG_CONSOLE_VGA_MULTI
        default 0
        export always
        comment "Multi VGA console"
end
define CONFIG_CONSOLE_VGA_ONBOARD_AT_FIRST
        default 0
        export always
        comment "Use onboard VGA instead of add on VGA card"
end
define CONFIG_CONSOLE_BTEXT
        default 0
        export always
        comment "Log messages to btext fb console"
end
define CONFIG_CONSOLE_LOGBUF
	default 0
	export always
	comment "Log messages to buffer"
end
define CONFIG_CONSOLE_SROM
	default 0
	export always
	comment "Log messages to SROM console"
end
define CONFIG_CONSOLE_SERIAL8250
	default 0
	export always
	comment "Log messages to 8250 uart based serial console"
end
define CONFIG_USBDEBUG_DIRECT
	default 0
	export always
	comment "Log messages to ehci debug port console"
end
define DEFAULT_CONSOLE_LOGLEVEL
	default 7
	export always
	comment "Console will log at this level unless changed"
end
define MAXIMUM_CONSOLE_LOGLEVEL
	default 8
	export always
 	comment "Error messages up to this level can be printed"
end
define CONFIG_SERIAL_POST
	default 0
	export always
	comment "Enable SERIAL POST codes"
end
define NO_POST
	default none
	export used
	comment "Disable POST codes"
end
define TTYS0_BASE
	default 0x3f8
	format "0x%x"
	export always
	comment "Base address for 8250 uart for the serial console"
end
define TTYS0_BAUD
	default 115200
	export always
	comment "Default baud rate for serial console"
end
define TTYS0_DIV
	default none
	format "%d"
	export used
	comment "Allow UART divisor to be set explicitly"
end
define TTYS0_LCS
	default 0x3
	format "0x%x"
	export always
	comment "Default flow control settings for the 8250 serial console uart"
end

define CONFIG_USE_PRINTK_IN_CAR
	default 0
	export always
	comment "use printk instead of print in CAR stage code"
end

	
###############################################
# Mainboard options
###############################################

define MAINBOARD
	default "Mainboard_not_set"
	export always
	comment "Mainboard name"
end
define MAINBOARD_PART_NUMBER
	default "Part_number_not_set"
	export always
	format "\"%s\""
	comment "Part number of mainboard"
end
define MAINBOARD_VENDOR
	default "Vendor_not_set"
	export always
	format "\"%s\""
	comment "Vendor of mainboard"
end
define MAINBOARD_PCI_SUBSYSTEM_VENDOR_ID
	default 0
	export always
	comment "PCI Vendor ID of mainboard manufacturer"
end
define MAINBOARD_PCI_SUBSYSTEM_DEVICE_ID
	default 0
	format "0x%x"
	export always
	comment "PCI susbsystem device id assigned my mainboard manufacturer"
end
define MAINBOARD_POWER_ON_AFTER_POWER_FAIL
	default none
	export used
	comment "Default power on after power fail setting"
end
define CONFIG_SYS_CLK_FREQ
	default none
	export used
	comment "System clock frequency in MHz"
end
define CONFIG_MAX_PCI_BUSES
	default 255
	export always
	comment "Maximum number of PCI buses to search for devices"
end
###############################################
# SMP options
###############################################

define CONFIG_SMP
	default 0
	export always
	comment "Define if we support SMP"
end
define CONFIG_MAX_CPUS
        default 1
        export always
        comment "Maximum CPU count for this machine"
end
define CONFIG_MAX_PHYSICAL_CPUS
        default 1
        export always
        comment "Maximum physical CPU count for this machine"
end
define CONFIG_LOGICAL_CPUS
	default 0
	export always
	comment "Should multiple cpus per die be enabled?"
end
define HAVE_MP_TABLE
	default none
	export used
	comment "Define to build an MP table"
end
define SERIAL_CPU_INIT
        default 1
        export always
        comment "Serialize CPU init"
end
define APIC_ID_OFFSET
	default 0
	export always
	comment "We need to share this value between cache_as_ram_auto.c and northbridge.c"
end
define ENABLE_APIC_EXT_ID
	default 0
	export always
	comment "Enable APIC ext id mode 8 bit"
end
define LIFT_BSP_APIC_ID
	default 0
	export always
	comment "decide if we lift bsp apic id while ap apic id"
end
###############################################
# Boot options
###############################################

define CONFIG_IDE_PAYLOAD
	default 0
	export always
	comment "Boot from IDE device"
end
define CONFIG_ROM_PAYLOAD
	default 0
	export always
	comment "Boot image is located in ROM" 
end
define CONFIG_ROM_PAYLOAD_START
	default {0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1}
	format "0x%x"
	export always
	comment "ROM stream start location"
end
define CONFIG_COMPRESSED_PAYLOAD_NRV2B
	default 0
	export always
	comment "NRV2B compressed boot image is located in ROM" 
end
define CONFIG_COMPRESSED_PAYLOAD_LZMA
	default 0
	export always
	comment "LZMA compressed boot image is located in ROM" 
end
define CONFIG_PRECOMPRESSED_PAYLOAD
	default 0
	export always
	comment "boot image is already compressed" 
end
define CONFIG_SERIAL_PAYLOAD
	default 0
	export always
	comment "Download boot image from serial port"
end
define CONFIG_FS_PAYLOAD
	default 0
	export always
	comment "Boot from a filesystem"
end
define CONFIG_FS_EXT2
	default 0
	export always
	comment "Enable ext2 filesystem support"
end
define CONFIG_FS_ISO9660
	default 0
	export always
	comment "Enable ISO9660 filesystem support"
end
define CONFIG_FS_FAT
	default 0
	export always
	comment "Enable FAT filesystem support"
end
define AUTOBOOT_DELAY
	default 2
	export always
	comment "Delay (in seconds) before autobooting"
end
define AUTOBOOT_CMDLINE
	default "hdc1:/vmlinuz root=/dev/hdc3 console=tty0 console=ttyS0,115200"
	export always
	format "\"%s\""
	comment "Default command line when autobooting"
end

define USE_WATCHDOG_ON_BOOT
	default 0
	export always
	comment "Use the watchdog on booting"
end

###############################################
# Plugin Device support options
###############################################

define CONFIG_HYPERTRANSPORT_PLUGIN_SUPPORT
	default 1
	export always
	comment "Enable support for plugin Hypertransport busses"
end
define CONFIG_AGP_PLUGIN_SUPPORT
	default 1
	export always
	comment "Enable support for plugin AGP busses"
end
define CONFIG_CARDBUS_PLUGIN_SUPPORT
	default 1
	export always
	comment "Enable support cardbus plugin cards"
end
define CONFIG_PCIX_PLUGIN_SUPPORT
	default 1
	export always
	comment "Enable support for plugin PCI-X busses"
end
define CONFIG_PCIEXP_PLUGIN_SUPPORT
	default 1
	export always
	comment "Enable support for plugin PCI-E busses"
end

###############################################
# IRQ options
###############################################

define HAVE_PIRQ_TABLE
	default none
	export used
	comment "Define if we have a PIRQ table"
end
define IRQ_SLOT_COUNT
	default none
	export used
	comment "Number of IRQ slots"
end
define CONFIG_PCIBIOS_IRQ
	default none
	export used
	comment "PCIBIOS IRQ support"
end
define CONFIG_IOAPIC
	default none
	export used
	comment "IOAPIC support"
end

###############################################
# IDE specific options
###############################################

define CONFIG_IDE
	default 0
	export always
	comment "Define to include IDE support"
end
define IDE_BOOT_DRIVE
	default 0
	export always
	comment "Disk number of boot drive"
end
define IDE_SWAB
	default none
	export used
	comment "Swap bytes when reading from IDE device"
end
define IDE_OFFSET
	default 0
	export always
	comment "Sector at which to start searching for boot image"
end

###############################################
# Options for memory mapped I/O
###############################################

define PCI_IO_CFG_EXT
	default 0
	export always
	comment "allow 4K register space via io CFG port"
end

define PCIC0_CFGADDR
	default none
	format "0x%x"
	export used
	comment "Address of PCI Configuration Address Register"
end
define PCIC0_CFGDATA
	default none
	format "0x%x"
	export used
	comment "Address of PCI Configuration Data Register"
end
define ISA_IO_BASE
	default none
	format "0x%x"
	export used
	comment "Base address of PCI/ISA I/O address range"
end
define ISA_MEM_BASE
	default none
	format "0x%x"
	export used
	comment "Base address of PCI/ISA memory address range"
end
define PNP_CFGADDR
	default none
	format "0x%x"
	export used
	comment "PNP Configuration Address Register offset"
end
define PNP_CFGDATA
	default none
	format "0x%x"
	export used
	comment "PNP Configuration Data Register offset"
end
define _IO_BASE
	default none
	format "0x%x"
	export used
	comment "Base address of memory mapped I/O operations"
end

###############################################
# Options for embedded systems
###############################################

define EMBEDDED_RAM_SIZE
	default none
	export used
	comment "Embedded boards generally have fixed RAM size"
end

###############################################
# Misc options
###############################################

define CONFIG_CHIP_NAME
	default 0
	export always
	comment "Compile in the chip name"
end

define CONFIG_GDB_STUB
	default 0
	export used
	comment "Compile in gdb stub support?"
end

define HAVE_INIT_TIMER
	default 0
	export always
	comment "Have a init_timer function"
end
define HAVE_HARD_RESET
	default none
	export used
	comment "Have hard reset"
end
define MEMORY_HOLE
	default none
	export used
	comment "Set to deal with memory hole"
end
define MAX_REBOOT_CNT
	default 3
	export always
	comment "Set maximum reboots"
end

###############################################
# Misc device options
###############################################

define CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2
	default 0
	export used
	comment "Use timer2 to callibrate the x86 time stamp counter"
end
define INTEL_PPRO_MTRR
	default none
	export used
	comment ""
end
define CONFIG_UDELAY_TSC
	default 0
	export used
	comment "Implement udelay with the x86 time stamp counter"
end
define CONFIG_UDELAY_IO
	default 0
	export used
	comment "Implement udelay with x86 io registers"
end
define FAKE_SPDROM
	default 0
	export always
	comment "Use this to fake spd rom values"
end

define HAVE_ACPI_TABLES
	default 0
	export always
	comment "Define to build ACPI tables"
end

define ACPI_SSDTX_NUM
	default 0
	export always
	comment "extra ssdt num for PCI Device"
end

define AGP_APERTURE_SIZE
	default none
	export used
	format "0x%x"
	comment "AGP graphics virtual memory aperture size"
end

define HT_CHAIN_UNITID_BASE
	default 1
	export always
	comment "this will be first hypertransport device's unitid base, if sb ht chain only has one ht device, it could be 0"
end

define HT_CHAIN_END_UNITID_BASE
        default 0x20
        export always
        comment "this will be unit id of the end of hypertransport chain (usually the real SB) if it is small than HT_CHAIN_UNITID_BASE, it could be 0"
end

define SB_HT_CHAIN_UNITID_OFFSET_ONLY
        default 1
        export always
        comment "this will decided if only offset SB hypertransport chain"
end

define SB_HT_CHAIN_ON_BUS0
        default 0 
        export always
        comment "this will make SB hypertransport chain sit on bus 0, if it is 1, will put sb ht chain on bus 0, if it is 2 will put other chain on 0x40, 0x80, 0xc0"
end

define PCI_BUS_SEGN_BITS
        default 0
        export always
        comment "It could be 0, 1, 2, 3 and 4 only"
end

define MMCONF_SUPPORT
	default 0
	export always
	comment "enable mmconfig for pci conf"
end

define MMCONF_SUPPORT_DEFAULT
	default 0
	export always
	comment "enable mmconfig for pci conf"
end

define HW_MEM_HOLE_SIZEK
        default 0
        export always
        comment "Opteron E0 later memory hole size in K, 0 mean disable"
end

define HW_MEM_HOLE_SIZE_AUTO_INC
        default 0
        export always
        comment "Opteron E0 later memory hole size auto increase to avoid hole startk equal to basek"
end

define CONFIG_VAR_MTRR_HOLE
	default 1
	export always
	comment "using hole in MTRR instead of increasing method"
end

define K8_HT_FREQ_1G_SUPPORT
	default 0 
	export always
	comment "Optern E0 later could support 1G HT, but still depends MB design"
end

define K8_REV_F_SUPPORT
        default 0
        export always
        comment "Opteron Rev F (DDR2) support"
end

define CBB
	default 0
	export always
	comment "Opteron cpu bus num base"
end

define CDB
	default 0x18
	export always
	comment "Opteron cpu device num base"
end

define HT3_SUPPORT
	default 0
	export always
	comment "Hypertransport 3 support, include ac HT and unganged sublink feature"
end

define EXT_RT_TBL_SUPPORT
	default 0
	export always
	comment "support AMD family 10 extended routing table via F0x158, normally is enabled when node nums is greater than 8"
end

define EXT_CONF_SUPPORT
	default 0
	export always
	comment "support AMD family 10 extended config space for ram, bus, io, mmio via F1x110, normally is enabled when HT3 is enabled and non ht chain nums is greater than 4"
end

define DIMM_SUPPORT
        default 0x0108
	format "0x%x"
        export always
        comment "DIMM support: bit 0 - sdram, bit 1: ddr1, bit 2: ddr2, bit 3: ddr3, bit 4: fbdimm, bit 8: reg"
end

define CPU_SOCKET_TYPE
	default 0x10
	export always
	comment "cpu socket type, 0x10 mean Socket F, 0x11 mean socket M2, 0x20, Soxket G, and 0x21 mean socket M3"
end

define CPU_ADDR_BITS
	default 36
	export always
	comment "CPU hardware address lines num, for AMD K8 could be 40, and AMD family 10 could be 48"
end

define CONFIG_VGA_ROM_RUN
	default 0
	export always
	comment "Init x86 ROMs on VGA-class PCI devices"
end

define CONFIG_PCI_ROM_RUN
	default 0
	export always
	comment "Init x86 ROMs on all PCI devices"
end

define CONFIG_PCI_64BIT_PREF_MEM
        default 0
        export always
        comment "allow PCI device get 4G above Region as pref mem"
end

define CONFIG_AMDMCT
	default 0
	export always
	comment "use AMD MCT to init RAM instead of native code"
end

define CONFIG_VIDEO_MB
        default none
        export used
        comment "Integrated graphics with UMA has dynamic setup"
end

define CONFIG_SPLASH_GRAPHIC
	default 0
	export used
	comment "Paint a splash screen"
end

define CONFIG_GX1_VIDEO
	default 0
	export used
	comment "Build in GX1's graphic support"
end

define CONFIG_GX1_VIDEOMODE
	default none
	export used
	comment "Define video mode after reset"
# could be
# 0 for 640x480
# 1 for 800x600
# 2 for 1024x768
# 3 for 1280x960
# 4 for 1280x1024
end

###############################################
# Board specific options
###############################################

###############################################
# Options for motorola/sandpoint
###############################################
define CONFIG_SANDPOINT_ALTIMUS
	default 0
	export never
	comment "Configure Sandpoint with Altimus PMC"
end
define CONFIG_SANDPOINT_TALUS
	default 0
	export never
	comment "Configure Sandpoint with Talus PMC"
end
define CONFIG_SANDPOINT_UNITY
	default 0
	export never
	comment "Configure Sandpoint with Unity PMC"
end
define CONFIG_SANDPOINT_VALIS
	default 0
	export never
	comment "Configure Sandpoint with Valis PMC"
end
define CONFIG_SANDPOINT_GYRUS
	default 0
	export never
	comment "Configure Sandpoint with Gyrus PMC"
end

###############################################
# Options for totalimpact/briq
###############################################
define CONFIG_BRIQ_750FX
	default 0
	export never
	comment "Configure briQ with PowerPC 750FX"
end
define CONFIG_BRIQ_7400
	default 0
	export never
	comment "Configure briQ with PowerPC G4"
end
