##
## This file is part of the coreboot project.
##
## Copyright (C) 2006 AMD
## Written by Yinghai Lu <yinghailu@gmail.com> for AMD.
##
## Copyright (C) 2006 MSI
## Written by Bingxun Shi <bingxunshi@gmail.com> for MSI.
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

##
## Compute the location and size of where this firmware image
## (coreboot plus bootloader) will live in the boot rom chip.
##
if USE_FALLBACK_IMAGE
       default ROM_SECTION_SIZE   = FALLBACK_SIZE
       default ROM_SECTION_OFFSET = ( ROM_SIZE - FALLBACK_SIZE )
else
       default ROM_SECTION_SIZE   = ( ROM_SIZE - FALLBACK_SIZE )
       default ROM_SECTION_OFFSET = 0
end

##
## Compute the start location and size size of
## The coreboot bootloader.
##
default PAYLOAD_SIZE            = ( ROM_SECTION_SIZE - ROM_IMAGE_SIZE )
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)
default CONFIG_ROM_PAYLOAD     = 1

##
## Compute where this copy of coreboot will start in the boot rom
##
default _ROMBASE      = ( CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE )

##
## Compute a range of ROM that can cached to speed up coreboot,
## execution speed.
##
## XIP_ROM_SIZE must be a power of 2.
## XIP_ROM_BASE must be a multiple of XIP_ROM_SIZE
##
default XIP_ROM_SIZE=65536
default XIP_ROM_BASE = ( _ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE )

arch i386 end


##
## Build the objects we have code for in this directory.
##

driver mainboard.o

#dir /drivers/ati/ragexl
#needed by irq_tables and mptable and acpi_tables
object get_bus_conf.o


if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
#object reset.o

if USE_DCACHE_RAM

if CONFIG_USE_INIT

makerule ./auto.o
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -o auto.o"
end

else

makerule ./auto.inc
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -S -o $@"
       action "perl -e 's/.rodata/.rom.data/g' -pi $@"
       action "perl -e 's/.text/.section .rom.text/g' -pi $@"
end

end
else

##
## Romcc output
##
makerule ./failover.E
        depends "$(MAINBOARD)/failover.c ./romcc"
        action "./romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./failover.inc
        depends "$(MAINBOARD)/failover.c ./romcc"
        action "./romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./auto.E
        depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
        action  "./romcc -E -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc
        depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
        action  "./romcc    -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end


end

##
## Build our 16 bit and 32 bit coreboot entry code
##
if USE_FALLBACK_IMAGE
        mainboardinit cpu/x86/16bit/entry16.inc
        ldscript /cpu/x86/16bit/entry16.lds
end

mainboardinit cpu/x86/32bit/entry32.inc

if USE_DCACHE_RAM
       if CONFIG_USE_INIT
               ldscript /cpu/x86/32bit/entry32.lds
       end

       if CONFIG_USE_INIT
               ldscript      /cpu/amd/car/cache_as_ram.lds
       end
end

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE
       mainboardinit cpu/x86/16bit/reset16.inc
       ldscript /cpu/x86/16bit/reset16.lds
else
       mainboardinit cpu/x86/32bit/reset32.inc
       ldscript /cpu/x86/32bit/reset32.lds
end

if USE_DCACHE_RAM
else
### Should this be in the northbridge code?
mainboardinit arch/i386/lib/cpu_reset.inc
end

##
## Include an id string (For safe flashing)
##
mainboardinit southbridge/nvidia/mcp55/id.inc
ldscript /southbridge/nvidia/mcp55/id.lds

##
## ROMSTRAP table for MCP55
##
if USE_FALLBACK_IMAGE
       mainboardinit southbridge/nvidia/mcp55/romstrap.inc
       ldscript /southbridge/nvidia/mcp55/romstrap.lds
end

if USE_DCACHE_RAM
##
## Setup Cache-As-Ram
##
mainboardinit cpu/amd/car/cache_as_ram.inc
end

###
### This is the early phase of coreboot startup
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
if USE_DCACHE_RAM
       ldscript /arch/i386/lib/failover.lds
else
       ldscript /arch/i386/lib/failover.lds
       mainboardinit ./failover.inc
end
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
if USE_DCACHE_RAM

if CONFIG_USE_INIT
initobject auto.o
else
mainboardinit ./auto.inc
end

else
# ROMCC
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit cpu/x86/sse/enable_sse.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/sse/disable_sse.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc

end

##
## Include the secondary Configuration files
##
if CONFIG_CHIP_NAME
        config chip.h
end


# sample config for msi/ms9282
chip northbridge/amd/amdk8/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_F
                        device apic 0 on end
                end
        end

       device pci_domain 0 on
               chip northbridge/amd/amdk8 #mc0
                       device pci 18.0 on #  northbridge
                               #  devices on link 0, link 0 == LDT 0
                               chip southbridge/nvidia/mcp55
                                       device pci 0.0 on end   # HT
                                       device pci 1.0 on # LPC
                                               chip superio/winbond/w83627ehg
                                                       device pnp 2e.0 on #  Floppy
                                                               io 0x60 = 0x3f0
                                                               irq 0x70 = 6
                                                               drq 0x74 = 2
                                                       end
                                                       device pnp 2e.1 off #  Parallel Port
                                                               io 0x60 = 0x378
                                                               irq 0x70 = 7
                                                       end
                                                       device pnp 2e.2 on #  Com1
                                                               io 0x60 = 0x3f8
                                                               irq 0x70 = 4
                                                       end
                                                       device pnp 2e.3 off #  Com2
                                                               io 0x60 = 0x2f8
                                                               irq 0x70 = 3
                                                       end
                                                       device pnp 2e.5 on #  Keyboard
                                                               io 0x60 = 0x60
                                                               io 0x62 = 0x64
                                                               irq 0x70 = 1
                                                               irq 0x72 = 12
                                                       end
                                                       device pnp 2e.6 off #  SERIAL_FALSH
                                                               io 0x60 = 0x100
                                                       end
                                                       device pnp 2e.7 off #  GAME_MIDI_GIPO1
                                                               io 0x60 = 0x220
                                                               io 0x62 = 0x300
                                                               irq 0x70 = 9
                                                       end
                                                       device pnp 2e.8 off end #  WDTO_PLED
                                                       device pnp 2e.9 off end #  GPIO2_GPIO3_GPIO4_GPIO5
                                                       device pnp 2e.a off end #  ACPI
                                                       device pnp 2e.b on #  HW Monitor
                                                               io 0x60 = 0x290
                                                               irq 0x70 = 5
                                                       end
                                               end
                                       end
                                        device pci 1.1 on # SM 0
                                               chip drivers/i2c/i2cmux2 # pca9554 smbus mux
                                                       device i2c 70 on  #0 pca9554 1
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 50 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 51 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 52 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 53 on end
                                                                end
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 54 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 55 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 56 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 57 on end
                                                                end
                                                       end
                                                       device i2c 70 on  #0 pca9554 2
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 50 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 51 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 52 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 53 on end
                                                                end
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 54 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 55 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 56 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 57 on end
                                                                end
                                                       end
                                               end
                                       end
                                       device pci 1.1 on # SM 1
                                               chip drivers/i2c/i2cmux2 # pca9554 smbus mux
                                                       device i2c 72 on     #pca9554 channle1
                                                               chip drivers/i2c/adm1027   #HWM ADT7476 1
                                                                       device i2c 2e on end
                                                               end
                                                       end
                                                       device i2c 72 on     #pca9545 channel 2
                                                               chip drivers/i2c/adm1027   #HWM ADT7463
                                                                       device i2c 2e on end
                                                               end
                                                       end
                                                       device i2c 72 on end  #pca9545 channel 3
                                                       device i2c 72 on      #pca9545 channel 4
                                                               chip drivers/i2c/adm1027   #HWM ADT7476 2
                                                                       device i2c 2e on end
                                                               end
                                                       end
                                               end
                                       end

                                       device pci 2.0 on end # USB 1.1
                                       device pci 2.1 on end # USB 2
                                       device pci 4.0 on  end # IDE
                                               device pci 5.0 on  end # SATA 0
                                       device pci 5.1 on  end # SATA 1
                                       device pci 5.2 on  end # SATA 2
                                       device pci 6.0 on  #P2P
                                               chip drivers/pci/onboard
                                                       device pci 4.0 on end
                                                       register "rom_address" = "0xfff80000"
                                               end
                                       end # P2P
                                       device pci 7.0 on end # reserve
                                       device pci 8.0 on end # MAC0
                                       device pci 9.0 on end # MAC1
                                       device pci a.0 on
                                               device pci 0.0 on
                                                       chip drivers/pci/onboard
                                                               device pci 4.0 on end  #pci_E lan1
                                                               device pci 4.1 on end  #pci_E lan2
                                                       end
                                               end
                                       end # 0x376
                                               device pci b.0 on  end # PCI E 0x374
                                       device pci c.0 on  end
                                       device pci d.0 on   #SAS
                                               chip drivers/pci/onboard
                                                       device pci 0.0 on end
                                               end
                                       end # PCI E 1 0x378
                                       device pci e.0 on end # PCI E 0 0x375
                                       device pci f.0 on end   #PCI E 0x377  pci_E slot
                                       register "ide0_enable" = "1"
                                       register "ide1_enable" = "1"
                                       register "sata0_enable" = "1"
                                       register "sata1_enable" = "1"
                               end
                       end #  device pci 18.0
                       device pci 18.0 on end # Link 1
                       device pci 18.0 on end
                       device pci 18.1 on end
                       device pci 18.2 on end
                       device pci 18.3 on end
               end #mc0

       end # pci_domain

#        chip drivers/generic/debug
#                device pnp 0.0 off end
#                device pnp 0.1 off end
#                device pnp 0.2 off end
#                device pnp 0.3 off end
#                device pnp 0.4 off end
#              device pnp 0.5 on end
#        end
end # root_complex
