# abuild config file for EPIA-M

target via_epia-m
mainboard via/epia-m

option  MAXIMUM_CONSOLE_LOGLEVEL=8
option  DEFAULT_CONSOLE_LOGLEVEL=8
option  CONFIG_CONSOLE_SERIAL8250=1

__COMPRESSION__

option ROM_SIZE=256*1024

option HAVE_OPTION_TABLE=1
option CONFIG_ROM_PAYLOAD=1
option HAVE_FALLBACK_BOOT=1

###
### Compute the location and size of where this firmware image
### (coreboot plus bootloader) will live in the boot rom chip.
###
option FALLBACK_SIZE=131072

## Coreboot C code runs at this location in RAM
option _RAMBASE=0x00004000

#
# Via EPIA M
#
romimage "normal"
	option USE_FALLBACK_IMAGE=0
	option ROM_IMAGE_SIZE=64*1024
	option COREBOOT_EXTRA_VERSION=".0-Normal"
	payload __PAYLOAD__
end

romimage "fallback" 
	option USE_FALLBACK_IMAGE=1
	option ROM_IMAGE_SIZE=64*1024
	option COREBOOT_EXTRA_VERSION=".0-Fallback"
	payload __PAYLOAD__
end

buildrom ./coreboot.rom ROM_SIZE "normal" "fallback"
