# Config file for the digitallogic msm800sev

target msm800sev
mainboard digitallogic/msm800sev

option CONFIG_COMPRESSED_PAYLOAD_NRV2B=0

## ROM_SIZE is the total number of bytes allocated for coreboot use
## (normal AND fallback images and payloads).
## leave 36k for vsa 
##
option ROM_SIZE = 1024*1024 - 36 * 1024

## ROM_IMAGE_SIZE is the maximum number of bytes allowed for a coreboot image,
## not including any payload.
option ROM_IMAGE_SIZE=64*1024

option FALLBACK_SIZE = ROM_SIZE

option DEFAULT_CONSOLE_LOGLEVEL = 11
option MAXIMUM_CONSOLE_LOGLEVEL = 11
romimage "fallback" 
	option USE_FALLBACK_IMAGE=1
	option COREBOOT_EXTRA_VERSION=".0Fallback"
	payload ../payload.elf 
end

buildrom ./coreboot.rom ROM_SIZE  "fallback"
