uses CONFIG_SANDPOINT_ALTIMUS
uses CONFIG_SANDPOINT_TALUS
uses CONFIG_SANDPOINT_UNITY
uses CONFIG_SANDPOINT_VALIS
uses CONFIG_SANDPOINT_GYRUS
uses ISA_IO_BASE
uses ISA_MEM_BASE
uses PCIC0_CFGADDR
uses PCIC0_CFGDATA
uses PNP_CFGADDR
uses PNP_CFGDATA
uses _IO_BASE

uses CROSS_COMPILE 
uses HAVE_OPTION_TABLE
uses CONFIG_SANDPOINT_ALTIMUS 
uses CONFIG_COMPRESS 
uses DEFAULT_CONSOLE_LOGLEVEL 
uses CONFIG_USE_INIT
uses CONFIG_CHIP_CONFIGURE
uses NO_POST
uses CONFIG_CONSOLE_SERIAL8250 
uses TTYS0_BASE 
uses CONFIG_IDE
uses CONFIG_FS_PAYLOAD 
uses CONFIG_FS_EXT2
uses CONFIG_FS_ISO9660
uses CONFIG_FS_FAT
uses AUTOBOOT_CMDLINE
uses PAYLOAD_SIZE
uses ROM_SIZE
uses ROM_IMAGE_SIZE
uses _RESET
uses _EXCEPTION_VECTORS
uses _ROMBASE
uses _ROMSTART
uses _RAMBASE
uses _RAMSTART
uses STACK_SIZE
uses HEAP_SIZE

uses MAINBOARD
uses MAINBOARD_VENDOR
uses MAINBOARD_PART_NUMBER
uses LINUXBIOS_EXTRA_VERSION
uses CROSS_COMPILE
uses CC
uses HOSTCC
uses OBJCOPY

##
## Set memory map
##
default ISA_IO_BASE=0xfe000000
default ISA_MEM_BASE=0xfd000000
default PCIC0_CFGADDR=0xfec00000
default PCIC0_CFGDATA=0xfee00000
default PNP_CFGADDR=0x15c
default PNP_CFGDATA=0x15d
default _IO_BASE=ISA_IO_BASE


## use a cross compiler
#default CROSS_COMPILE="powerpc-eabi-"
#default CROSS_COMPILE="ppc_74xx-"

## Use stage 1 initialization code
default CONFIG_USE_INIT=1

## Use static configuration
default CONFIG_CHIP_CONFIGURE=1

## We don't use compressed image
default CONFIG_COMPRESS=0

## Turn off POST codes
default NO_POST=1

## Enable serial console
default DEFAULT_CONSOLE_LOGLEVEL=8
default CONFIG_CONSOLE_SERIAL8250=1
default TTYS0_BASE=0x3f8

## Load payload using filo
default CONFIG_IDE=1
default CONFIG_FS_PAYLOAD=1
default CONFIG_FS_EXT2=1
default CONFIG_FS_ISO9660=1
default CONFIG_FS_FAT=1
default AUTOBOOT_CMDLINE="hdc1:/vmlinuz"

# LinuxBIOS must fit into 128KB
default ROM_IMAGE_SIZE=131072
default ROM_SIZE={ROM_IMAGE_SIZE+PAYLOAD_SIZE}
default PAYLOAD_SIZE=262144

# Set stack and heap sizes (stage 2)
default STACK_SIZE=0x10000
default HEAP_SIZE=0x10000

# Sandpoint Demo Board
## Base of ROM
default _ROMBASE=0xfff00000

## Sandpoint reset vector
default _RESET=_ROMBASE+0x100

## Exception vectors (other than reset vector)
default _EXCEPTION_VECTORS=_RESET+0x100

## Start of linuxBIOS in the boot rom
## = _RESET + exeception vector table size
default _ROMSTART=_RESET+0x3100

## LinuxBIOS C code runs at this location in RAM
default _RAMBASE=0x00100000
default _RAMSTART=0x00100000

default CONFIG_SANDPOINT_ALTIMUS=1

### End Options.lb
end
