##
## Compute the location and size of where this firmware image
## (linuxBIOS plus bootloader) will live in the boot rom chip.
##
if USE_FALLBACK_IMAGE
	default ROM_SECTION_SIZE   = FALLBACK_SIZE
	default ROM_SECTION_OFFSET = ( ROM_SIZE - FALLBACK_SIZE )
else
	default ROM_SECTION_SIZE   = ( ROM_SIZE - FALLBACK_SIZE )
	default ROM_SECTION_OFFSET = 0
end

##
## Compute the start location and size size of
## The linuxBIOS bootloader.
##
default PAYLOAD_SIZE            = ( ROM_SECTION_SIZE - ROM_IMAGE_SIZE )
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)

##
## Compute where this copy of linuxBIOS will start in the boot rom
##
default _ROMBASE      = ( CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE )

##
## Compute a range of ROM that can cached to speed up linuxBIOS,
## execution speed.
##
## XIP_ROM_SIZE must be a power of 2.
## XIP_ROM_BASE must be a multiple of XIP_ROM_SIZE
##
default XIP_ROM_SIZE=65536
default XIP_ROM_BASE = ( _ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE )

arch i386 end 

##
## Build the objects we have code for in this directory.
##

driver mainboard.o
if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
#object reset.o

##
## Romcc output
##
makerule ./failover.E
	depends "$(MAINBOARD)/failover.c ./romcc" 
	action "./romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./failover.inc
	depends "$(MAINBOARD)/failover.c ./romcc"
	action "./romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./auto.E 
	depends	"$(MAINBOARD)/auto.c option_table.h ./romcc" 
	action	"./romcc -E -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc 
	depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
	action	"./romcc    -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end

##
## Build our 16 bit and 32 bit linuxBIOS entry code
##
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
ldscript /cpu/x86/32bit/entry32.lds

##
## Build our reset vector (This is where linuxBIOS is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc
	ldscript /cpu/x86/16bit/reset16.lds
else
	mainboardinit cpu/x86/32bit/reset32.inc
	ldscript /cpu/x86/32bit/reset32.lds
end

### Should this be in the northbridge code?
mainboardinit arch/i386/lib/cpu_reset.inc

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

###
### This is the early phase of linuxBIOS startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
	ldscript /arch/i386/lib/failover.lds 
	mainboardinit ./failover.inc
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit cpu/x86/sse/enable_sse.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/sse/disable_sse.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc
 
##
## Include the secondary Configuration files 
##
dir /pc80
config chip.h

chip northbridge/amd/amdk8/root_complex
	device pci_domain 0 on
		chip northbridge/amd/amdk8 # mc
			device pci 18.0 on end # LDT 0 
			device pci 18.0 on end # LDT1
			device pci 18.0 on     # LDT2
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device	pnp 2e.0 on  # Floppy 
								 io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off  # Parallel Port
								 io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 on # Com 1
								 io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.3 off # Com 2
								 io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.5 on  # Keyboard
								 io 0x60 = 0x60
								 io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.6 off end # CIR
							device pnp 2e.7 off end # GAM_MIDI_GIPO1
							device pnp 2e.8 off end # GPIO2
							device pnp 2e.9 off end # GPIO3
							device pnp 2e.a off end # ACPI
							device pnp 2e.b on      # HW Monitor
								 io 0x60 = 0x290
							end 
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 off end
					device pci 1.6 off end
                                        register "ide0_enable" = "1"
                                        register "ide1_enable" = "1"
				end
			end # device pci 18.0 
			
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
		chip northbridge/amd/amdk8
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.1 on end
			device pci 19.2 on end
			device pci 19.3 on end
		end
	end
	device apic_cluster 0 on
		chip cpu/amd/socket_940
			device apic 0 on end
		end
		chip cpu/amd/socket_940
			device apic 1 on end
		end
	end
end

