uses HAVE_MP_TABLE
uses HAVE_ACPI_TABLES
uses HAVE_PIRQ_TABLE
uses HAVE_FALLBACK_BOOT
uses HAVE_OPTION_TABLE
uses IRQ_SLOT_COUNT
uses CONFIG_MAX_CPUS
uses CONFIG_LOGICAL_CPUS
uses CONFIG_MAX_PHYSICAL_CPUS
uses CONFIG_IOAPIC
uses CONFIG_SMP
uses CONFIG_ROM_PAYLOAD
uses CONFIG_COMPRESSED_PAYLOAD_LZMA
uses STACK_SIZE
uses HEAP_SIZE
uses USE_OPTION_TABLE
uses LB_CKS_RANGE_START
uses LB_CKS_RANGE_END
uses LB_CKS_LOC
uses MAINBOARD_PART_NUMBER
uses MAINBOARD_VENDOR
uses MAINBOARD
uses MAINBOARD_PCI_SUBSYSTEM_VENDOR_ID
uses MAINBOARD_PCI_SUBSYSTEM_DEVICE_ID
uses _RAMBASE
uses TTYS0_BAUD
uses TTYS0_BASE
uses TTYS0_LCS
uses DEFAULT_CONSOLE_LOGLEVEL
uses MAXIMUM_CONSOLE_LOGLEVEL
uses MAINBOARD_POWER_ON_AFTER_POWER_FAIL
uses CONFIG_CONSOLE_SERIAL8250
uses CONFIG_UDELAY_TSC
uses CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2
uses HAVE_INIT_TIMER
uses CONFIG_GDB_STUB
uses CROSS_COMPILE
uses CC
uses HOSTCC
uses OBJCOPY
uses CONFIG_CHIP_NAME
uses CONFIG_CONSOLE_VGA
uses CONFIG_PCI_ROM_RUN
uses DEBUG
#uses CPU_OPT
uses CONFIG_IDE

## The default definitions are used for these
uses CONFIG_ROM_PAYLOAD_START
uses PAYLOAD_SIZE

## These are defined in target Config.lb, don't add here
uses USE_FALLBACK_IMAGE
uses ROM_SIZE
uses ROM_IMAGE_SIZE
uses FALLBACK_SIZE
uses LINUXBIOS_EXTRA_VERSION

## These are defined in mainboard Config.lb, don't add here
uses ROM_SECTION_SIZE
uses ROM_SECTION_OFFSET
uses _ROMBASE
uses XIP_ROM_SIZE
uses XIP_ROM_BASE

###
### Build options
###

##
## ROM_SIZE is the size of boot ROM that this board will use.
##
default ROM_SIZE=2097152
default ROM_IMAGE_SIZE = 65536

##
## Build code for the fallback boot?
##
default HAVE_FALLBACK_BOOT=1
default FALLBACK_SIZE=131072


## Delay timer options
##
default CONFIG_UDELAY_TSC=1
default CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2=1

##
## Build code to export a programmable irq routing table
##
default HAVE_PIRQ_TABLE=1
default IRQ_SLOT_COUNT=12

##
## Build code to export an x86 MP table
## Useful for specifying IRQ routing values
##
default HAVE_MP_TABLE=1

## Build code to export ACPI tables?
default HAVE_ACPI_TABLES=1

##
## Build code to export a CMOS option table?
##
default HAVE_OPTION_TABLE=0

## CMOS checksum definitions (units == bytes)
## These must match the checksum record in cmos.layout
default LB_CKS_RANGE_START=128
default LB_CKS_RANGE_END=130
default LB_CKS_LOC=131

##
## Build code for SMP support
## Only worry about 2 micro processors
## NOTE: CONFIG_MAX_CPUS is the number of LOGICAL CPUs,
##		 so if CONFIG_LOGICAL_CPUS is 1, CONFIG_MAX_CPUS should be 4.
##
default CONFIG_SMP=1
default CONFIG_MAX_CPUS=2
default CONFIG_LOGICAL_CPUS=0
default CONFIG_MAX_PHYSICAL_CPUS=2

# VGA Console
# NOTE: to initialize VGA, need to copy the VGA option ROM from the factory BIOS
#	    to VGA.rom
default CONFIG_CONSOLE_VGA=0
default CONFIG_PCI_ROM_RUN=0

##
## Build code to setup a generic IOAPIC
##
default CONFIG_IOAPIC=1

##
## Motherboard identification
##
default MAINBOARD_PART_NUMBER="EIDXE7501DEVKIT"
default MAINBOARD_VENDOR="Intel"
default MAINBOARD_PCI_SUBSYSTEM_VENDOR_ID=0x8086
default MAINBOARD_PCI_SUBSYSTEM_DEVICE_ID=0x2480

###
### LinuxBIOS layout values
###

##
## Use a small 8K stack
##
default STACK_SIZE=0x2000

##
## Use a small 16K heap
##
default HEAP_SIZE=0x4000

##
## CMOS settings not currently supported due to conflicts with factory BIOS
##
default USE_OPTION_TABLE = 0

##
## LinuxBIOS C code runs at this location in RAM
##
default _RAMBASE=0x00004000

##
## Load the payload from the ROM
##
default CONFIG_ROM_PAYLOAD = 1

###
### Defaults of options that you may want to override in the target config file
### 

##
## The default compiler
##
default CC="$(CROSS_COMPILE)gcc -m32"
default HOSTCC="gcc"

##
## Disable the gdb stub by default
## 
default CONFIG_GDB_STUB=0

##
## The Serial Console
##

# To Enable the Serial Console
default CONFIG_CONSOLE_SERIAL8250=1

## Select the serial console baud rate
default TTYS0_BAUD=115200
#default TTYS0_BAUD=57600
#default TTYS0_BAUD=38400
#default TTYS0_BAUD=19200
#default TTYS0_BAUD=9600
#default TTYS0_BAUD=4800
#default TTYS0_BAUD=2400
#default TTYS0_BAUD=1200

# Select the serial console base port
default TTYS0_BASE=0x3f8

# Select the serial protocol
# This defaults to 8 data bits, 1 stop bit, and no parity
default TTYS0_LCS=0x3

##
### Select the linuxBIOS loglevel
##
## EMERG      1   system is unusable               
## ALERT      2   action must be taken immediately 
## CRIT       3   critical conditions              
## ERR        4   error conditions                 
## WARNING    5   warning conditions               
## NOTICE     6   normal but significant condition 
## INFO       7   informational                    
## DEBUG      8   debug-level messages             
## SPEW       9   Way too many details             

## Request this level of debugging output
default  DEFAULT_CONSOLE_LOGLEVEL=8
## At a maximum only compile in this level of debugging
default  MAXIMUM_CONSOLE_LOGLEVEL=8

##
## Select power on after power fail setting
default MAINBOARD_POWER_ON_AFTER_POWER_FAIL="MAINBOARD_POWER_ON"

## Things we may not have
default CONFIG_IDE=1

default DEBUG=1
# default CPU_OPT="-g"
default CONFIG_CHIP_NAME=1

### End Options.lb
end
