##
## This file is part of the coreboot project.
##
## Copyright (C) 2007 Uwe Hermann <uwe@hermann-uwe.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

uses HAVE_MP_TABLE
uses CONFIG_CBFS
uses HAVE_PIRQ_TABLE
uses USE_FALLBACK_IMAGE
uses HAVE_FALLBACK_BOOT
uses HAVE_HARD_RESET
uses HAVE_OPTION_TABLE
uses USE_OPTION_TABLE
uses CONFIG_ROM_PAYLOAD
uses IRQ_SLOT_COUNT
uses MAINBOARD
uses MAINBOARD_VENDOR
uses MAINBOARD_PART_NUMBER
uses COREBOOT_EXTRA_VERSION
uses ARCH
uses FALLBACK_SIZE
uses STACK_SIZE
uses HEAP_SIZE
uses ROM_SIZE
uses ROM_SECTION_SIZE
uses ROM_IMAGE_SIZE
uses ROM_SECTION_SIZE
uses ROM_SECTION_OFFSET
uses CONFIG_ROM_PAYLOAD_START
uses CONFIG_COMPRESSED_PAYLOAD_LZMA
uses PAYLOAD_SIZE
uses _ROMBASE
uses _RAMBASE
uses XIP_ROM_SIZE
uses XIP_ROM_BASE
uses HAVE_MP_TABLE
uses CROSS_COMPILE
uses CC
uses HOSTCC
uses OBJCOPY
uses DEFAULT_CONSOLE_LOGLEVEL
uses MAXIMUM_CONSOLE_LOGLEVEL
uses CONFIG_CONSOLE_SERIAL8250
uses TTYS0_BAUD
uses TTYS0_BASE
uses TTYS0_LCS
uses CONFIG_UDELAY_TSC
uses CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2
uses MAINBOARD_VENDOR
uses MAINBOARD_PART_NUMBER
uses CONFIG_CONSOLE_VGA
uses CONFIG_PCI_ROM_RUN

default ROM_SIZE = 512 * 1024		# Override this in targets/*/Config.lb.
default HAVE_FALLBACK_BOOT = 1
default HAVE_MP_TABLE = 0
default HAVE_HARD_RESET = 0
default CONFIG_UDELAY_TSC = 1
default CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2 = 1
default HAVE_PIRQ_TABLE = 1
default IRQ_SLOT_COUNT = 0		# Override this in targets/*/Config.lb.
default MAINBOARD_VENDOR = "N/A"	# Override this in targets/*/Config.lb.
default MAINBOARD_PART_NUMBER = "N/A"	# Override this in targets/*/Config.lb.
default ROM_IMAGE_SIZE = 64 * 1024
default FALLBACK_SIZE = 128 * 1024
default STACK_SIZE = 8 * 1024
default HEAP_SIZE = 16 * 1024
default HAVE_OPTION_TABLE = 0
#default USE_OPTION_TABLE = !USE_FALLBACK_IMAGE
default USE_OPTION_TABLE = 0
default _RAMBASE = 0x00004000
default CONFIG_ROM_PAYLOAD = 1
default CROSS_COMPILE = ""
default CC = "$(CROSS_COMPILE)gcc -m32"
default HOSTCC = "gcc"
default CONFIG_CONSOLE_SERIAL8250 = 1
default TTYS0_BAUD = 115200
default TTYS0_BASE = 0x3f8
default TTYS0_LCS = 0x3			# 8n1
default DEFAULT_CONSOLE_LOGLEVEL = 9	# Override this in targets/*/Config.lb.
default MAXIMUM_CONSOLE_LOGLEVEL = 9	# Override this in targets/*/Config.lb.
default CONFIG_CONSOLE_VGA = 1		# Override this in targets/*/Config.lb.
default CONFIG_PCI_ROM_RUN = 1		# Override this in targets/*/Config.lb.

#
# CBFS
#
#
default CONFIG_CBFS=0
end
