##
## Config file for the Total Impact briQ
##

##
## Early board initialization, called from ppc_main()
##
initobject init.o
initobject clock.o

##
## Stage 2 timer support
##
object clock.o

arch ppc end

if CONFIG_BRIQ_750FX
dir /cpu/ppc/ppc7xx
end
if CONFIG_BRIQ_7400
dir /cpu/ppc/mpc74xx
end

##
## Include the secondary Configuration files 
##
chip northbridge/ibm/cpc710
	device pci_domain 0 on # 32bit pci bridge
		device pci 0.0 on 
			chip southbridge/winbond/w83c553
				# FIXME  The function numbers are ok but the device id is wrong here!
				device pci 0.0 on end # pci to isa bridge
				device pci 0.1 on end # pci ide controller
			end
		end
	end
	device cpu_bus 0 on 
	#	chip cpu/ppc/ppc7xx
	#		device cpu 0 on end
	#	end
	end
end

##
## Build the objects we have code for in this directory.
##

addaction coreboot.a "$(CROSS_COMPILE)ranlib coreboot.a"
