chip northbridge/amd/amdk8/root_complex
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on end # LDT 0
			device pci 18.0 on     # LDT 1
				chip southbridge/amd/amd8131
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/nsc/pc87366
							device	pnp 2e.0 off  # Floppy 
								 io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off  # Parallel Port
								 io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 off # Com 2
								 io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.3 on  # Com 1
								 io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.4 off end # SWC
							device pnp 2e.5 off end # Mouse
							device pnp 2e.6 on  # Keyboard
								 io 0x60 = 0x60
								 io 0x62 = 0x64
								irq 0x70 = 1
							end
							device pnp 2e.7 off end # GPIO
							device pnp 2e.8 off end # ACB
							device pnp 2e.9 off end # FSCM
							device pnp 2e.a off end # WDT  
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 off end
					device pci 1.6 off end
				end
			end #  device pci 18.0 
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
		chip northbridge/amd/amdk8
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.1 on end
			device pci 19.2 on end
			device pci 19.3 on end
		end
	end 
	device apic_cluster 0 on
		chip cpu/amd/socket_940
			device apic 0 on end
		end
		chip cpu/amd/socket_940
			device apic 1 on end
		end
	end
end

