<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="22" y1="-1.27" x2="37" y2="-1.27" width="0" layer="20"/>
<wire x1="37" y1="-1.27" x2="37" y2="13" width="0" layer="20"/>
<wire x1="37" y1="13" x2="42.079" y2="13" width="0" layer="20"/>
<wire x1="42.079" y1="13" x2="42.079" y2="40.0254" width="0" layer="20"/>
<wire x1="42.079" y1="40.0254" x2="21.4572" y2="40.0254" width="0" layer="20"/>
<wire x1="21.4572" y1="40.0254" x2="21.4572" y2="44.222" width="0" layer="20"/>
<wire x1="21.4572" y1="44.222" x2="13.2032" y2="44.222" width="0" layer="20"/>
<wire x1="13.2032" y1="44.222" x2="13.2032" y2="31.623" width="0" layer="20"/>
<wire x1="13.2032" y1="31.623" x2="22.86" y2="31.623" width="0" layer="20"/>
<wire x1="22.86" y1="31.623" x2="24.13" y2="30.353" width="0" layer="20"/>
<wire x1="24.13" y1="30.353" x2="24.13" y2="16.508" width="0" layer="20"/>
<wire x1="24.13" y1="16.508" x2="16.492" y2="16.508" width="0" layer="20"/>
<wire x1="16.492" y1="16.508" x2="16.492" y2="13.4412" width="0" layer="20"/>
<wire x1="16.492" y1="13.4412" x2="19.3396" y2="13.4412" width="0" layer="20"/>
<wire x1="19.3396" y1="13.4412" x2="19.3396" y2="10.492" width="0" layer="20"/>
<wire x1="19.3396" y1="10.492" x2="22" y2="10.492" width="0" layer="20"/>
<wire x1="22" y1="10.492" x2="22" y2="-1.27" width="0" layer="20"/>
<text>A0</text>
<text>USB mod for
Power Replay

bit.ly/pcsx-redux</text>
</plain>
<libraries>
<library name="Wurth_EMC Components_WE-VE">
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - ESD Protection - WE-VE&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-VE_0603">
<description>&lt;B&gt;WE-VE ESD Suppressor
&lt;BR&gt;&lt;/B&gt;Size : 0603
&lt;br&gt;L X W X H = 1.6mm X 0.8mm X 1.6mm</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
</packages>
</library>
<library name="SparkFun-Coils">
<description>&lt;h3&gt;SparkFun Coils&lt;/h3&gt;
In this library you'll find magnetics.

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Inductors&lt;/li&gt;
&lt;li&gt;Ferrite Beads&lt;/li&gt;
&lt;li&gt;Transformers&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;br&gt;
&lt;p&gt;We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.&lt;/p&gt;</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pixel">
<packages>
<package name="BUFFER-CASTELLATION">
</package>
<package name="TSSOP14-RU">
<description>&lt;b&gt;14-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] (RU-14)&lt;p&gt;
Source: www.analog.com .. OP1177_2177_4177.pdf</description>
</package>
<package name="QFN48_8MM">
</package>
<package name="PLA-CASTELLATION">
<description>&lt;b&gt;PLCC&lt;/b&gt;&lt;p&gt;
20 lead square</description>
</package>
<package name="SMD3225-4P">
</package>
<package name="0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="0402">
<description>&lt;b&gt; 0402&lt;/b&gt;</description>
</package>
<package name="1206">
</package>
<package name="TP">
</package>
<package name="USB-C">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DDP" library="Wurth_EMC Components_WE-VE" package="WE-VE_0603" value="5V">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/82356050050.pdf"/>
<attribute name="ILEAK" value="1uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82356050050 "/>
<attribute name="RISO" value="10  MOhm "/>
<attribute name="VALUE"/>
<attribute name="VCLAMP-TYP" value="75V"/>
<attribute name="VESD-AIR" value="15kV"/>
</element>
<element name="DDM" library="Wurth_EMC Components_WE-VE" package="WE-VE_0603" value="5V">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/82356050050.pdf"/>
<attribute name="ILEAK" value="1uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82356050050 "/>
<attribute name="RISO" value="10  MOhm "/>
<attribute name="VALUE"/>
<attribute name="VCLAMP-TYP" value="75V"/>
<attribute name="VESD-AIR" value="15kV"/>
</element>
<element name="EEPROM" library="microchip" package="SOT23-6" value="93LC76B">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="93LC76BT-I/OT"/>
<attribute name="OC_FARNELL" value="1556170"/>
<attribute name="OC_NEWARK" value="61H6848"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="FBPLL" library="SparkFun-Coils" package="0603" value="600Ω/0.5A">
<attribute name="PROD_ID" value="NDUC-07859"/>
<attribute name="VALUE"/>
</element>
<element name="FBPHY" library="SparkFun-Coils" package="0603" value="600Ω/0.5A">
<attribute name="PROD_ID" value="NDUC-07859"/>
<attribute name="VALUE"/>
</element>
<element name="FVBUS" library="SparkFun-Coils" package="0603" value="600Ω/0.5A">
<attribute name="PROD_ID" value="NDUC-07859"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI" library="pixel" package="QFN48_8MM" value="FT232HQFN">
<attribute name="VALUE"/>
</element>
<element name="CAST1" library="pixel" package="BUFFER-CASTELLATION" value="BUFFER-CASTELLATION"/>
<element name="GATES" library="pixel" package="TSSOP14-RU" value="7402TSSOP14">
<attribute name="VALUE"/>
</element>
<element name="CAST2" library="pixel" package="PLA-CASTELLATION" value="PLA-CASTELLATION">
<attribute name="VALUE"/>
</element>
<element name="XTAL" library="pixel" package="SMD3225-4P" value="CRYSTAL"/>
<element name="CPLL" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="CPHY" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="CVBUS" library="pixel" package="1206" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="REE" library="pixel" package="0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="RRESET" library="pixel" package="0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="RREF" library="pixel" package="0603" value="12k">
<attribute name="VALUE"/>
</element>
<element name="CX1" library="pixel" package="0402" value="27pF">
<attribute name="VALUE"/>
</element>
<element name="CX2" library="pixel" package="0402" value="27pF">
<attribute name="VALUE"/>
</element>
<element name="CVCCA" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="CVCORE" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="CRESET" library="pixel" package="0603" value="10nF">
<attribute name="VALUE"/>
</element>
<element name="CVCC" library="pixel" package="1206" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="C1" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="pixel" package="0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="TP" library="pixel" package="TP" value="TP"/>
<element name="USB" library="pixel" package="USB-C" value="">
<attribute name="VALUE"/>
</element>
<element name="RCC1" library="pixel" package="0402" value="5.1k">
<attribute name="VALUE"/>
</element>
<element name="RCC2" library="pixel" package="0402" value="5.1k">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="EEPROM" pad="2"/>
<contactref element="CAST1" pad="P$9"/>
<contactref element="GATES" pad="7"/>
<contactref element="CPLL" pad="2"/>
<contactref element="CPHY" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="CVCC" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="USB" pad="M1"/>
<contactref element="USB" pad="M3"/>
<contactref element="USB" pad="M2"/>
<contactref element="USB" pad="A1B12"/>
<contactref element="USB" pad="B1A12"/>
<contactref element="USB" pad="M4"/>
<contactref element="DDP" pad="2"/>
<contactref element="DDM" pad="2"/>
<contactref element="FTDI" pad="42"/>
<contactref element="FTDI" pad="10"/>
<contactref element="FTDI" pad="11"/>
<contactref element="FTDI" pad="22"/>
<contactref element="FTDI" pad="23"/>
<contactref element="FTDI" pad="35"/>
<contactref element="FTDI" pad="36"/>
<contactref element="FTDI" pad="47"/>
<contactref element="FTDI" pad="48"/>
<contactref element="FTDI" pad="4"/>
<contactref element="FTDI" pad="9"/>
<contactref element="FTDI" pad="41"/>
<contactref element="FTDI" pad="THERMAL"/>
<contactref element="XTAL" pad="P$2"/>
<contactref element="XTAL" pad="P$4"/>
<contactref element="CVBUS" pad="2"/>
<contactref element="RREF" pad="1"/>
<contactref element="CX1" pad="2"/>
<contactref element="CX2" pad="2"/>
<contactref element="CVCCA" pad="2"/>
<contactref element="CVCORE" pad="2"/>
<contactref element="CRESET" pad="2"/>
<contactref element="RCC1" pad="2"/>
<contactref element="RCC2" pad="2"/>
</signal>
<signal name="EECS">
<contactref element="EEPROM" pad="5"/>
<contactref element="FTDI" pad="45"/>
</signal>
<signal name="EECLK">
<contactref element="EEPROM" pad="4"/>
<contactref element="FTDI" pad="44"/>
</signal>
<signal name="EEDATA">
<contactref element="EEPROM" pad="3"/>
<contactref element="FTDI" pad="43"/>
<contactref element="REE" pad="2"/>
</signal>
<signal name="EEDO">
<contactref element="EEPROM" pad="1"/>
<contactref element="REE" pad="1"/>
</signal>
<signal name="REF">
<contactref element="FTDI" pad="5"/>
<contactref element="RREF" pad="2"/>
</signal>
<signal name="!RESET_FT">
<contactref element="FTDI" pad="34"/>
<contactref element="CRESET" pad="1"/>
<contactref element="RRESET" pad="2"/>
</signal>
<signal name="VPLL">
<contactref element="FBPLL" pad="2"/>
<contactref element="FTDI" pad="8"/>
<contactref element="CPLL" pad="1"/>
</signal>
<signal name="VPHY">
<contactref element="FBPHY" pad="2"/>
<contactref element="FTDI" pad="3"/>
<contactref element="CPHY" pad="1"/>
</signal>
<signal name="DM">
<contactref element="DDM" pad="1"/>
<contactref element="FTDI" pad="6"/>
<contactref element="USB" pad="A7"/>
<contactref element="USB" pad="B7"/>
</signal>
<signal name="DP">
<contactref element="DDP" pad="1"/>
<contactref element="FTDI" pad="7"/>
<contactref element="USB" pad="B6"/>
<contactref element="USB" pad="A6"/>
</signal>
<signal name="VBUS">
<contactref element="FVBUS" pad="1"/>
<contactref element="USB" pad="A4B9"/>
<contactref element="USB" pad="B4A9"/>
</signal>
<signal name="VREGIN">
<contactref element="FVBUS" pad="2"/>
<contactref element="FTDI" pad="40"/>
<contactref element="CVBUS" pad="1"/>
</signal>
<signal name="RWR">
<contactref element="GATES" pad="13"/>
<contactref element="GATES" pad="2"/>
<contactref element="GATES" pad="3"/>
</signal>
<signal name="RRD">
<contactref element="GATES" pad="10"/>
<contactref element="GATES" pad="5"/>
<contactref element="GATES" pad="6"/>
</signal>
<signal name="5V">
<contactref element="CAST1" pad="P$11"/>
<contactref element="GATES" pad="14"/>
</signal>
<signal name="OE">
<contactref element="CAST1" pad="P$10"/>
<contactref element="FTDI" pad="21"/>
<contactref element="GATES" pad="11"/>
<contactref element="GATES" pad="9"/>
</signal>
<signal name="RD+CS">
<contactref element="FTDI" pad="26"/>
<contactref element="GATES" pad="4"/>
</signal>
<signal name="WR+CS">
<contactref element="FTDI" pad="27"/>
<contactref element="GATES" pad="1"/>
</signal>
<signal name="D0">
<contactref element="FTDI" pad="13"/>
<contactref element="CAST1" pad="P$1"/>
</signal>
<signal name="D1">
<contactref element="CAST1" pad="P$2"/>
<contactref element="FTDI" pad="14"/>
</signal>
<signal name="D2">
<contactref element="FTDI" pad="15"/>
<contactref element="CAST1" pad="P$3"/>
</signal>
<signal name="D3">
<contactref element="CAST1" pad="P$4"/>
<contactref element="FTDI" pad="16"/>
</signal>
<signal name="D4">
<contactref element="FTDI" pad="17"/>
<contactref element="CAST1" pad="P$5"/>
</signal>
<signal name="D5">
<contactref element="CAST1" pad="P$6"/>
<contactref element="FTDI" pad="18"/>
</signal>
<signal name="D6">
<contactref element="FTDI" pad="19"/>
<contactref element="CAST1" pad="P$7"/>
</signal>
<signal name="D7">
<contactref element="CAST1" pad="P$8"/>
<contactref element="FTDI" pad="20"/>
</signal>
<signal name="WR">
<contactref element="CAST2" pad="P$1"/>
<contactref element="GATES" pad="12"/>
</signal>
<signal name="RD">
<contactref element="CAST2" pad="P$2"/>
<contactref element="GATES" pad="8"/>
</signal>
<signal name="XO">
<contactref element="CX2" pad="1"/>
<contactref element="XTAL" pad="P$3"/>
<contactref element="FTDI" pad="2"/>
</signal>
<signal name="XI">
<contactref element="FTDI" pad="1"/>
<contactref element="XTAL" pad="P$1"/>
<contactref element="CX1" pad="1"/>
</signal>
<signal name="VCCA">
<contactref element="FTDI" pad="37"/>
<contactref element="CVCCA" pad="1"/>
</signal>
<signal name="VCORE">
<contactref element="FTDI" pad="38"/>
<contactref element="CVCORE" pad="1"/>
</signal>
<signal name="A0">
<contactref element="FTDI" pad="25"/>
<contactref element="TP" pad="P$1"/>
</signal>
<signal name="+3V3">
<contactref element="FBPHY" pad="1"/>
<contactref element="FBPLL" pad="1"/>
<contactref element="FTDI" pad="12"/>
<contactref element="FTDI" pad="24"/>
<contactref element="FTDI" pad="46"/>
<contactref element="FTDI" pad="39"/>
<contactref element="CVCC" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="EEPROM" pad="6"/>
<contactref element="RRESET" pad="1"/>
</signal>
<signal name="CC1">
<contactref element="USB" pad="A5"/>
<contactref element="RCC1" pad="1"/>
</signal>
<signal name="CC2">
<contactref element="USB" pad="B5"/>
<contactref element="RCC2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
